{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKCBX-BBV3"]
[]
[]
[]
[]
["","","","","EKCBX008BBV3"]
["Wymiary","Jednostka","Szerokość","mm","412"]
["","","Głębokość z modułem Remocon zamontowanym na panelu przednim","mm","120"]
["","","Głębokość","mm","100"]
["","","Wysokość","mm","390"]
["Ciężar","Jednostka","","kg","6"]
["Element grzejny urządzenia wspomagającego","Zasilanie","Faza","","1~, 3~"]
["","","Napięcie","V","230, 400"]
["","","Częstotliwość","Hz","50"]
["Uwagi","","","","(1) - Wspomniane powyżej zasilanie skrzynki hydraulicznej jest przeznaczone tylko dla dodatkowego elementu grzejnego. Skrzynka rozdzielcza i pompa hydroboxu zasilane są przez jednostkę zewnętrzną. Opcjonalny zbiornik ciepłej wody użytkowej ma oddzielne źródło zasilania."]
["","","","","(2) - W zależności od ustawienia priorytetu zapasowego elementu grzewczego zestaw grzejnika zapasowego EKMBUH* może lub nie może pracować równocześnie."]
["","","","","(3) - Więcej szczegółów można znaleźć w instrukcji instalacji EBHQ*; specyfikacje dla zestawu zapasowego elementu grzewczego można znaleźć w specyfikacjach EKMBUH*"]
["","","","","(4) - Złącza przewodów: wybierz średnicę i typ zgodnie z miejscowymi przepisami. Więcej informacji na temat zakresu napięcia i prądu można znaleźć w instrukcji instalacji EBHQ*"]
["","","","","(5) - Zasilanie odnosi się do kombinacji odpowiednio z EKHW*V3 i EKHW*Z2."]