{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":7,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHH2E-AV3"]
[]
[]
[]
[]
["","","","","","EKHH2E200AAV3","EKHH2E260AAV3"]
["Sound power level","Domestic hot water heating","","Indoor unit","dBA","53","53"]
["","","","Outdoor unit","dBA","52","52"]
["Podgrzewanie ciepłej wody użytkowej","Informacje ogólne","","Klasa efektywności energetycznej podgrzewu wody","","A+","A+"]
["","","","Ustawienie temperatury na termostacie","°C","55","55"]
["","","","Zadeklarowany profil obciążenia","","L","XL"]
["","Zimny klimat","","AEC (roczne zużycie energii)","kWh","1,091","1,826"]
["","Ciepły klimat","","AEC (roczne zużycie energii)","kWh","756","1,296"]
["","Klimat umiarkowany","","AEC (roczne zużycie energii)","kWh","835","1,323"]
["Equivalent hot water","Max","","","l","275","342"]
["Pompa ciepła","Automatyczne uruchomienie odszraniania","","","°C","-2","-2"]
["","Zakres pracy","Temp. otoczenia","Min.","°CDB","-7","-7"]
["","","","Maks.","°CDB","38","38"]
["","Obudowa","","Materiał","","Pokrywa: Wykończenie górnej części z EPP","Pokrywa: Wykończenie górnej części z EPP"]
["","","","Colour","","White body / black top","White body / black top"]
["","Ciśnienie w układzie","","Maks.","bar","7","7"]
["","Metoda odszraniania","","","","Aktywna z zaworem gorącego gazu","Aktywna z zaworem gorącego gazu"]
["COP","","","","","2.94 (1), 3.30 (2)","3.10 (1), 3.60 (2)"]
["Czynnik chłodniczy","GWP","","","","1,430.0","1,430.0"]
["","Dopełnienie","","","kg","0.900","0.900"]
["","Typ","","","","R-134a","R-134a"]
["Sprężarka","Typ","","","","Rotary non-inverter","Rotary non-inverter"]
["Wymiary","Jednostka","","Średnica","mm","650","650"]
["","","","Wysokość","mm","1,714","2,000"]
["Ciepła woda użytkowa","Moc wyjściowa","","Nom.","kW","1.8","1.8"]
["Zbiornik","Installation","","Solar thermal connection possible","","Nie","Nie"]
["","Integrated heating element power","","Nom.","kW","1.5","1.5"]
["","Obudowa","","Materiał","","Wygniatany ABS","Wygniatany ABS"]
["","","","Kolor","","Biały","Biały"]
["","Wymiary","Jednostka","Wysokość","mm","1,210","1,500"]
["","Zakres pracy","Strona wodna","Maks.","°C","56","56"]
["","","","Min.","°C","10","10"]
["Ciężar","Jednostka zapakowana","","","kg","103","115"]
["","Jednostka","","Pusty","kg","83","95"]
["","","","Pełna","kg","282","349"]
["Miejsce instalacji","","","","","Jednostka wewnętrzna","Jednostka wewnętrzna"]
["Klasa IP","","","","","IP-X4","IP-X4"]
["General","Product description","","Pompa ciepła powietrze-woda","","Tak","Tak"]
["","Szczegółowe dane dostawcy/producenta","","Nazwa i adres","","ELIC - Via Pietro Zorutti 13/14, 33074 Fontanafredda ITALY","ELIC - Via Pietro Zorutti 13/14, 33074 Fontanafredda ITALY"]
["Heat up time","Max.","","","hh:mm","08:17:00, 06:30:44","10:14:00, 07:56:46"]
["Pompa ciepła","Zasilanie","","Częstotliwość","Hz","50","50"]
["","","","Maksymalny prąd roboczy","A","2","2"]
["","","","Faza","","1P","1P"]
["","","","Napięcie","V","230","230"]
["Zbiornik","Zasilanie","","Faza","","1P","1P"]
["","","","Częstotliwość","Hz","50","50"]
["","","","Napięcie","V","230","230"]
["Uwagi","","","","","(1) - Zgodnie z EN16147-2011, temperatura wlotowa 7°C, temperatura w pomieszczeniu 20°C, temperatura wlotowa zimnej wody 10°C","(1) - Zgodnie z EN16147-2011, temperatura wlotowa 7°C, temperatura w pomieszczeniu 20°C, temperatura wlotowa zimnej wody 10°C"]
["","","","","","(2) - Zgodnie z EN16147-2011, temperatura wlotowa 15°C, temperatura w pomieszczeniu 20°C, temperatura wlotowa zimnej wody 10°C","(2) - Zgodnie z EN16147-2011, temperatura wlotowa 15°C, temperatura w pomieszczeniu 20°C, temperatura wlotowa zimnej wody 10°C"]
["","","","","","(3) - Temperatura wewnątrz pomieszczeń: 29°CDB, 19°CWB; temp. zewnętrzna: 46°CDB, 24°CWB","(3) - Temperatura wewnątrz pomieszczeń: 29°CDB, 19°CWB; temp. zewnętrzna: 46°CDB, 24°CWB"]
["","","","","","(4) - Temperatura wewnątrz pomieszczeń: 27°CDB, 19°CWB; temp. zewnętrzna: 35°CDB, 24°CWB","(4) - Temperatura wewnątrz pomieszczeń: 27°CDB, 19°CWB; temp. zewnętrzna: 35°CDB, 24°CWB"]