{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":102,"n_cols":7,"rows_kept":102,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHH2E-AV33"]
[]
[]
[]
[]
["","","","","","EKHH2E200AAV33","EKHH2E260AAV33"]
["Poziom mocy akustycznej","Podgrzewanie ciepłej wody użytkowej","","Jednostka wewnętrzna","dBA","","53"]
["","","","Outdoor unit","dBA","","52"]
["Ciepła woda użytkowa i grzanie","Informacje ogólne","","Klasa efektywności energetycznej podgrzewu wody","","","A+"]
["","","","Ustawienie temperatury na termostacie","°C","","55"]
["","","","Zadeklarowany profil obciążenia","","","XL"]
["","Klimat zimny","","AEC (roczne zużycie energii)","kWh","","1,826"]
["","Klimat ciepły","","AEC (roczne zużycie energii)","kWh","","1,296"]
["","Klimat umiarkowany","","AEC (roczne zużycie energii)","kWh","","1,323"]
["Równoważna objętość wody gorącej","Maks.","","","l","","342"]
["Pompa ciepła","Automatic defrost start","","","°C","","-2"]
["","Zakres pracy","Temp. otoczenia","Min.","°CDB","","-7"]
["","","","Maks.","°CDB","","38"]
["","Casing","","Material","","","Pokrywa: Wykończenie górnej części z EPP"]
["","","","Kolor","","","White body / black top"]
["","Ciśnienie w układzie","","Maks.","bar","","7"]
["","Metoda odszraniania","","","","","Aktywna z zaworem gorącego gazu"]
["COP","","","","","3.30 (2), 2.88 (1)","3.10 (1), 3.60 (2)"]
["Czynnik chłodniczy","GWP","","","","","1,430.0"]
["","Ilość","","","kg","","0.900"]
["","Typ","","","","","R-134a"]
["Compressor","Type","","","","","Rotary non-inverter"]
["Wymiary","Jednostka","","Średnica","mm","","650"]
["","","","Wysokość","mm","","2,000"]
["Ciepła woda użytkowa","Moc wyjściowa","","Nom.","kW","","1.8"]
["Zbiornik","Instalacja","","Możliwość wykorzystania solarnego wspomagania termicznego","","","Nie"]
["","Moc zintegrowanego elementu grzewczego","","Nom.","kW","","1.5"]
["","Obudowa","","Materiał","","","Wygniatany ABS"]
["","","","Kolor","","","Biały"]
["","Wymiary","Jednostka","Wysokość","mm","","1,500"]
["","Zakres pracy","Strona wodna","Maks.","°C","","56"]
["","","","Min.","°C","","10"]
["Ciężar","Jednostka zapakowana","","","kg","","115"]
["","Jednostka","","Pusty","kg","","95"]
["","","","Pełna","kg","","349"]
["Miejsce instalacji","","","","","","Jednostka wewnętrzna"]
["Klasa IP","","","","","","IP-X4"]
["Informacje ogólne","Opis produktu","","Pompa ciepła powietrze-woda","","","Tak"]
["","Szczegółowe dane dostawcy/producenta","","Nazwa i adres","","","ELIC - Via Pietro Zorutti 13/14, 33074 Fontanafredda ITALY"]
["Czas rozgrzewania","Maks.","","","hh:mm","","10:14:00, 07:56:46"]
["Pompa ciepła","Zasilanie","","Częstotliwość","Hz","","50"]
["","","","Maksymalny prąd roboczy","A","","2"]
["","","","Faza","","","1P"]
["","","","Napięcie","V","","230"]
["Zbiornik","Zasilanie","","Faza","","","1P"]
["","","","Częstotliwość","Hz","","50"]
["","","","Napięcie","V","","230"]
["Uwagi","","","","","(1) - Zgodnie z EN16147-2011, temperatura wlotowa 7°C, temperatura w pomieszczeniu 20°C, temperatura wlotowa zimnej wody 10°C","(1) - Zgodnie z EN16147-2011, temperatura wlotowa 7°C, temperatura w pomieszczeniu 20°C, temperatura wlotowa zimnej wody 10°C"]
["","","","","","(2) - Zgodnie z EN16147-2011, temperatura wlotowa 15°C, temperatura w pomieszczeniu 20°C, temperatura wlotowa zimnej wody 10°C","(2) - Zgodnie z EN16147-2011, temperatura wlotowa 15°C, temperatura w pomieszczeniu 20°C, temperatura wlotowa zimnej wody 10°C"]
["","","","","","","(3) - Temperatura wewnątrz pomieszczeń: 29°CDB, 19°CWB; temp. zewnętrzna: 46°CDB, 24°CWB"]
["","","","","","","(4) - Temperatura wewnątrz pomieszczeń: 27°CDB, 19°CWB; temp. zewnętrzna: 35°CDB, 24°CWB"]
["Czas rozgrzewania","Maks.","","","hh:mm","08:17:00, 06:30:44"]
["Ciepła woda użytkowa","Moc wyjściowa","","Nom.","kW","1.8"]
["Równoważna objętość wody gorącej","Maks.","","","l","275"]
["Wymiary","Jednostka","","Wysokość","mm","1714"]
["wymiary","Jednostka","","Średnica","mm","650"]
["Ciężar","Jednostka","","Pusty","kg","83"]
["","","","Pełna","kg","282"]
["","Jednostka zapakowana","","","kg","103"]
["Miejsce instalacji","","","","","Jednostka wewnętrzna"]
["Klasa IP","","","","","IP-X4"]
["Sprężarka","Typ","","","","Rotacyjna bez inwertera"]
["Czynnik chłodniczy","Typ","","","","R-134a"]
["","GWP","","","","1430.0"]
["","Ilość","","","tCO2Eq","1.29"]
["","Ilość","","","kg","0.900"]
["Pompa ciepła","Obudowa","","Kolor","","Biały korpus / czarna górna część"]
["","","","Pompa ciepła-=-Obudowa-=-Materiał","","Pokrywa: Wykończenie górnej części z EPP"]
["","Zakres pracy","Temp. otoczenia","Min.","°CDB","-7"]
["","","","Maks.","°CDB","38"]
["","Metoda odszraniania","","","","Aktywna z zaworem gorącego gazu"]
["","Automatyczne uruchomienie odszraniania","","","°C","-2"]
["","Ciśnienie w układzie","","Maks.","bar","7"]
["Zbiornik","Zakres pracy","Strona wodna","Maks.","°C","56"]
["","","","Min.","°C","10"]
["","Moc zintegrowanego elementu grzewczego","","Nom.","kW","1.5"]
["","Obudowa","","Kolor","","Biały"]
["","","","Materiał","","Wygniatany ABS"]
["","Wymiary","Jednostka","Wysokość","mm","1210"]
["","Instalacja","","Możliwość wykorzystania solarnego wspomagania termicznego","","Nie"]
["Informacje ogólne","Opis produktu","","Pompa ciepła powietrze-woda","","Tak"]
["Ogólny","Szczegółowe dane dostawcy/producenta","","Nazwa i adres","","ELIC - Via Pietro Zorutti 13/14, 33074 Fontanafredda ITALY"]
["Ciepła woda użytkowa i grzanie","Informacje ogólne","","Zadeklarowany profil obciążenia","","L"]
["Podgrzew ciepłej wody użytkowej","Informacje ogólne","","Klasa efektywności energetycznej podgrzewu wody","","A+"]
["Podgrzewanie ciepłej wody użytkowej","Ogólny","","Ustawienie temperatury na termostacie","°C","55"]
["Poziom mocy akustycznej","Podgrzewanie ciepłej wody użytkowej","","Jednostka zewnętrzna","dBA","52"]
["","","","Jednostka wewnętrzna","dBA","53"]
["Ciepła woda użytkowa i grzanie","Klimat umiarkowany","","AEC (roczne zużycie energii)","kWh","835"]
["","Klimat zimny","","AEC (roczne zużycie energii)","kWh","1091"]
["","Klimat ciepły","","AEC (roczne zużycie energii)","kWh","756"]
["Pompa ciepła","Zasilanie","","Faza","","1P"]
["","","","Częstotliwość","Hz","50"]
["","","","Napięcie","V","230"]
["","","","Maksymalny prąd roboczy","A","2"]
["Zbiornik","Zasilanie","","Faza","","1P"]
["","","","Częstotliwość","Hz","50"]
["","","","Napięcie","V","230"]