{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":6,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHH2E-PAV33"]
[]
[]
[]
[]
["","","","","","EKHH2E260PAAV33"]
["Czas rozgrzewania","Maks.","","","hh:mm","10:14:00, 07:56:46"]
["COP","","","","","3.10, 3.60"]
["Ciepła woda użytkowa","Moc wyjściowa","","Nom.","kW","1.8"]
["Równoważna objętość wody gorącej","Maks.","","","l","342"]
["Wymiary","Jednostka","","Wysokość","mm","2000"]
["wymiary","Jednostka","","Średnica","mm","650"]
["Ciężar","Jednostka","","Pusty","kg","112"]
["","","","Pełna","kg","358"]
["","Jednostka zapakowana","","","kg","132"]
["Miejsce instalacji","","","","","Jednostka wewnętrzna"]
["Klasa IP","","","","","IP-X4"]
["Sprężarka","Typ","","","","Rotacyjna bez inwertera"]
["Czynnik chłodniczy","Typ","","","","R-134a"]
["","GWP","","","","1430.0"]
["","Ilość","","","tCO2Eq","1.29"]
["","Ilość","","","kg","0.900"]
["Pompa ciepła","Obudowa","","Kolor","","Biały korpus / czarna górna część"]
["","","","Pompa ciepła-=-Obudowa-=-Materiał","","Pokrywa: Wykończenie górnej części z EPP"]
["","Zakres pracy","Temp. otoczenia","Min.","°CDB","-7"]
["","","","Maks.","°CDB","38"]
["","Metoda odszraniania","","","","Aktywna z zaworem gorącego gazu"]
["","Automatyczne uruchomienie odszraniania","","","°C","-2"]
["","Ciśnienie w układzie","","Maks.","bar","7"]
["Zbiornik","Zakres pracy","Strona wodna","Maks.","°C","56"]
["","","","Min.","°C","10"]
["","Moc zintegrowanego elementu grzewczego","","Nom.","kW","1.5"]
["","Obudowa","","Kolor","","Biały"]
["","","","Materiał","","Wygniatany ABS"]
["","Wymiary","Jednostka","Wysokość","mm","1500"]
["","Instalacja","","Możliwość wykorzystania solarnego wspomagania termicznego","","Tak"]
["Informacje ogólne","Opis produktu","","Pompa ciepła powietrze-woda","","Tak"]
["Ogólny","Szczegółowe dane dostawcy/producenta","","Nazwa i adres","","ELIC - Via Pietro Zorutti 13/14, 33074 Fontanafredda ITALY"]
["Ciepła woda użytkowa i grzanie","Informacje ogólne","","Zadeklarowany profil obciążenia","","XL"]
["Podgrzew ciepłej wody użytkowej","Informacje ogólne","","Klasa efektywności energetycznej podgrzewu wody","","A+"]
["Podgrzewanie ciepłej wody użytkowej","Ogólny","","Ustawienie temperatury na termostacie","°C","55"]
["Poziom mocy akustycznej","Podgrzewanie ciepłej wody użytkowej","","Jednostka zewnętrzna","dBA","52"]
["","","","Jednostka wewnętrzna","dBA","53"]
["Ciepła woda użytkowa i grzanie","Klimat umiarkowany","","AEC (roczne zużycie energii)","kWh","1323"]
["","Klimat zimny","","AEC (roczne zużycie energii)","kWh","1826"]
["","Klimat ciepły","","AEC (roczne zużycie energii)","kWh","1296"]
["Zakres efektywności energetycznej","","","","","A+ ~ F"]
["Pompa ciepła","Zasilanie","","Faza","","1P"]
["","","","Częstotliwość","Hz","50"]
["","","","Napięcie","V","230"]
["","","","Maksymalny prąd roboczy","A","2"]
["Zbiornik","Zasilanie","","Faza","","1P"]
["","","","Częstotliwość","Hz","50"]
["","","","Napięcie","V","230"]
["Uwagi","","","","","(1) - Zgodnie z EN16147-2011, temperatura wlotowa 7°C, temperatura w pomieszczeniu 20°C, temperatura wlotowa zimnej wody 10°C"]
["","","","","","(2) - Zgodnie z EN16147-2011, temperatura wlotowa 15°C, temperatura w pomieszczeniu 20°C, temperatura wlotowa zimnej wody 10°C"]