{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":10,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHHP-A2V3"]
[]
[]
[]
[]
["","","","","EKHHP300AC2V3","EKHHP500AC2V3","EKHHP500AA2V3 (Archived)","EKHHP500AB2V3 (Archived)","EKHHP300AA2V3 (Archived)","EKHHP300AB2V3 (Archived)"]
["Poziom ciś. akust.","Nom.","","dBA","0","0","0","0","0","0"]
["Czynnik chłodniczy","GWP","","","2,087.5","2,087.5","","2,087.5","","2,087.5"]
["","Typ","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Poziom mocy akustycznej","Nom.","","dBA","39","39","0","39","0","39"]
["Wymiary","Jednostka","Szerokość","mm","595","790","790","790","615","595"]
["","","Głębokość","mm","615","790","790","790","615","615"]
["","","Wysokość","mm","1,772","1,778","1,750","1,778","1,750","1,772"]
["Obudowa","Colour","","","Biały (RAL9016) / Ciemno-szary (RAL7011)","Biały (RAL9016) / Ciemno-szary (RAL7011)","Biały (RAL9016) / Ciemno-szary (RAL7011)","Biały (RAL9016) / Ciemno-szary (RAL7011)","Biały (RAL9016) / Ciemno-szary (RAL7011)","Biały (RAL9016) / Ciemno-szary (RAL7011)"]
["PED","Kategoria","","","Kategoria I","Kategoria I","Kategoria I","Kategoria I","Kategoria I","Kategoria I"]
["Ciężar","Jednostka","","kg","70","80","80","80","70","70"]
["Power supply","Phase","","","1~","1~","3N~","1~","3N~","1~"]
["","Częstotliwość","","Hz","50","50","50","50","50","50"]
["","Napięcie","","V","230","230","230","230","230","230"]
["Prąd","zalecane bezpieczniki","","A","16","16","16","16","16","16"]
["Uwagi","","","","(1) - Straty ciepła według EN12897","(1) - Straty ciepła według EN12897","","(1) - Straty ciepła według EN12897","","(1) - Straty ciepła według EN12897"]