{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":7,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWET-BV3"]
[]
[]
[]
[]
["","","","","","EKHWET90BAV3","EKHWET120BAV3"]
["Montaż","","","","","Ściana","Ściana"]
["Obudowa","Kolor","","","","BIAŁY +CZARNY","BIAŁY +CZARNY"]
["","Materiał","","","","blacha cienka, Tworzywo akrylonitrylo-butadieno-styrenowe","blacha cienka, Tworzywo akrylonitrylo-butadieno-styrenowe"]
["Wymiary","Jednostka","Wysokość","Zbiornik","mm","1032","1283"]
["","","","Szerokość","mm","510","510"]
["","","","Głębokość","mm","570","570"]
["Ciężar","Jednostka","","Pusty","kg","43","47"]
["Zbiornik","Objętość wody","","","l","89","118"]
["","Materiał","","","","Stal emaliowana według DIN4753TL2","Stal emaliowana według DIN4753TL2"]
["","Maksymalna temperatura wody","","","°C","75.0","75.0"]
["","Klasa efektywności energetycznej","","","","B","C"]
["Wymiennik ciepła","Ciepła woda użytkowa","","Ilość","","1","1"]
["","","","Materiał rury","","Aluminium","Aluminium"]
["","","","Ciśnienie operacyjne","bar","42","42"]
["Element grzejny booster","Wydajność","","","kW","1.2","1.2"]