{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":5,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKMBDXA"]
[]
[]
[]
[]
["","","","","EKMBDXA7V1"]
["Maks. liczba możliwych do podłączenia jedn. wewnętrznych","","","","64"]
["Komunikacja","DIII-NET","Uwaga","","DIII-NET (F1F2)"]
["Instalacja","","","","Instalacja w pomieszczeniu"]
["Wymiary","Jednostka","Szerokość","mm","379"]
["","","Głębokość","mm","87"]
["","","Wysokość","mm","124"]
["Ciężar","Jednostka","","kg","2.1"]
["Maks. liczba możliwych do podłączenia jedn. zewnętrznych","","","","10"]
["Power supply","Częstotliwość","","Hz","50"]
["","Napięcie","","V","220-240"]