{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":5,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKRTR"]
[]
[]
[]
[]
["","","","","EKRTR1"]
["Funkcja regulacji","","","","Zakres proporcjonalności"]
["Wymiary","Odbiornik","Wysokość","mm","170"]
["","","Głębokość","mm","28"]
["","","Szerokość","mm","50"]
["","Termostat","Głębokość","mm","34"]
["","","Szerokość","mm","125"]
["","","Wysokość","mm","87"]
["Zakres nastawy temperatur","Ogrzewanie","Maks.","°C","37"]
["","","Min.","°C","4"]
["","Chłodzenie","Maks.","°C","37"]
["","","Min.","°C","4"]
["Zegar","","","","Tak"]
["Ciężar","Odbiornik","","g","125"]
["","Termostat","","g","210"]
["Temperatura otoczenia","Przechowywanie","Maks.","°F","140"]
["","","Min.","°C","-20"]
["","","Maks.","°C","60"]
["","","Min.","°F","-4"]
["","Działanie","Min.","°C","0"]
["","","Maks.","°F","122"]
["","","Min.","°F","32"]
["","","Maks.","°C","50"]
["Maksymalny znamionowy prąd przełączenia (przy 230 V AC)","A","","","4.0 (1)"]
["Maksymalna odległość od odbiornika","Na zewnątrz","","m","około 100 m"]
["","Wewnątrz","","m","około 30 m"]
["Złącze","Termostat","","","Bezprzewodowy"]
["","Odbiornik","","","Przewodowy"]
["Power supply","liczba faz","","","1~"]
["","Częstotliwość","","Hz","50"]
["","Odbiornik","Napięcie","V","230"]
["","Termostat","Napięcie","V","Zasilana 3 bateriami AA-LR6 (alkaliczne)"]
["Uwagi","","","","(1) - 230VAC"]