{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":5,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKRTW"]
[]
[]
[]
[]
["","","","","EKRTWA"]
["Funkcja regulacji","","","","Zakres proporcjonalności"]
["Wymiary","Jednostka","Szerokość","mm","125"]
["","","Głębokość","mm","34"]
["","","Wysokość","mm","87"]
["Zakres nastawy temperatur","Ogrzewanie","Maks.","°C","37"]
["","","Min.","°C","4"]
["","Chłodzenie","Maks.","°C","37"]
["","","Min.","°C","4"]
["Zegar","","","","Tak"]
["Ciężar","Jednostka","","g","215"]
["Temperatura otoczenia","Przechowywanie","Min.","°C","-20"]
["","","Maks.","°F","140"]
["","","Min.","°F","-4"]
["","","Maks.","°C","60"]
["","Działanie","Min.","°C","0"]
["","","Maks.","°F","122"]
["","","Min.","°F","32"]
["","","Maks.","°C","50"]
["Maksymalny znamionowy prąd przełączenia (przy 230 V AC)","A","","","5.0 (1)"]
["Złącze","Typ","","","Z przewodem"]
["Power supply","Napięcie","","V","Zasilana 3* bateriami AA-LR6 (alkaliczne)"]
["Uwagi","","","","(1) - 230VAC"]