{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":8,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKSV-P"]
[]
[]
[]
[]
["","","","","EKSV21P","EKSV21P1","EKSV26P","EKSV26P1"]
["Pochłaniacz","","","","Rura miedziana o ostrych kształtach ze spawaną laserowo o wysokim stopniu selektywności płytą aluminiową","Rura miedziana o ostrych kształtach ze spawaną laserowo o wysokim stopniu selektywności płytą aluminiową","Rura miedziana o ostrych kształtach ze spawaną laserowo o wysokim stopniu selektywności płytą aluminiową","Rura miedziana o ostrych kształtach ze spawaną laserowo o wysokim stopniu selektywności płytą aluminiową"]
["Temperatura w stanie spoczynku","Maks.","","°C","192","192","192","192"]
["Wymiary","Jednostka","Szerokość","mm","85","1,006","85","1,300"]
["","","Głębokość","mm","2,000","85","2,000","85"]
["","","Wysokość","mm","1,006","2,000","1,300","2,000"]
["Ciśnienie operacyjne","Maks.","","bar","6","6","6","6"]
["Ciężar","Jednostka","","kg","33","35","42","42"]
["Powierzchnia","Otwór","","m²","1.800","1.800","2.360","2.360"]
["","Pochłaniacz","","m²","1.79","1.80","2.35","2.36"]
["","Zewnętrzna","","m²","2.01","2.01","2.60","2.60"]
["Montaż","","","","W pionie","W pionie","W pionie","W pionie"]
["Szkliwienie","","","","Jedno-taflowe szkło bezodpryskowe, transmisja +/- 92%","Jedno-taflowe szkło bezodpryskowe, transmisja +/- 92%","Jedno-taflowe szkło bezodpryskowe, transmisja +/- 92%","Jedno-taflowe szkło bezodpryskowe, transmisja +/- 92%"]
["Dopuszczalny kąt dachu","Maks.","","°","80","80","80","80"]
["","Min.","","°","15","15","15","15"]
["Powłoka","","","","Micro-therm (absorpcja maks. 96%, emisja ok.  5% +/-2%)","Micro-therm (absorpcja maks. 96%, emisja ok.  5% +/-2%)","Micro-therm (absorpcja maks. 96%, emisja ok.  5% +/-2%)","Micro-therm (absorpcja maks. 96%, emisja ok.  5% +/-2%)"]
["Objętość","l","","","1.3","1.3","1.7","1.7"]
["Thermal performance","Zerowy współczynnik straty kolektora η0","","%","0.781","0.710","0.784","0.710"]
["","Współczynnik straty ciepła a1","","W/m².K","4.240","4.300","4.250","4.300"]
["","Zależność temperatury od współczynnika straty ciepła a2","","W/m².K²","0.006","0.006","0.007","0.006"]
["","Wydajność cieplna","","kJ/K","4.9","4.9","6.5","6.5"]