{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELSX-E"]
[]
[]
[]
[]
["","","","","","ELSX12P50EG","ELSX12P30EG","ELSX12P50EF","ELSX12P30EF"]
["Obudowa","Kolor","","","","Biały (RAL9016) / Czarny (RAL9017)","Biały (RAL9016) / Czarny (RAL9017)","Biały (RAL9016) / Czarny (RAL9017)","Biały (RAL9016) / Czarny (RAL9017)"]
["","Materiał","","","","Polipropylen odporny na uderzenia","Polipropylen odporny na uderzenia","Polipropylen odporny na uderzenia","Polipropylen odporny na uderzenia"]
["Wymiary","Jednostka","","Wysokość","mm","1,910","1,891","1,910","1,893"]
["","","","Szerokość","mm","792","594","792","594"]
["","","","Głębokość","mm","817","680","817","680"]
["Ciężar","Jednostka","","","kg","112","91.0","91.0","76.0"]
["PED","Kategoria","","","","Kategoria II","Kategoria II","Kategoria II","Kategoria II"]
["Czynnik chłodniczy","Typ","","","","R-32","R-32","R-32","R-32"]
["Poziom mocy akustycznej","Nom.","","","dBA","44.7","44.7","44.7","44.7"]
["Poziom ciśnienia akustycznego","Nom.","","","dBA","36.8","36.8","36.8","36.8"]
["Zakres pracy","Grzanie","Strona wodna","Min.","°C","15 (3)","15 (3)","15 (3)","15 (3)"]
["","","","Maks.","°C","65 (3)","65 (3)","65 (3)","65 (3)"]
["","Chłodzenie","Temp. otoczenia","Min.","°CDB","10 (3)","10 (3)","10 (3)","10 (3)"]
["","","Strona wodna","Min.","°C","5 (3)","5 (3)","5 (3)","5 (3)"]
["","","","Maks.","°C","22 (3)","22 (3)","22 (3)","22 (3)"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50","50"]
["","Napięcie","","","V","230","230","230","230"]
["Uwagi","","","","","(1) - Obszar działania rozciąga się do niższych natężeń przepływu w zależności od trybu pracy - patrz krzywa ESP.","(1) - Obszar działania rozciąga się do niższych natężeń przepływu w zależności od trybu pracy - patrz krzywa ESP.","(1) - Obszar działania rozciąga się do niższych natężeń przepływu w zależności od trybu pracy - patrz krzywa ESP.","(1) - Obszar działania rozciąga się do niższych natężeń przepływu w zależności od trybu pracy - patrz krzywa ESP."]
["","","","","","(2) - Straty ciepła według EN12897","(2) - Straty ciepła według EN12897","(2) - Straty ciepła według EN12897","(2) - Straty ciepła według EN12897"]
["","","","","","(3) - Więcej szczegółów widać na rysunku zakresu pracy","(3) - Więcej szczegółów widać na rysunku zakresu pracy","(3) - Więcej szczegółów widać na rysunku zakresu pracy","(3) - Więcej szczegółów widać na rysunku zakresu pracy"]