{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EVH"]
[]
[]
[]
[]
["","","","","","ERGA06EAV3H"]
["Wymiary","Jednostka","","Wysokość","mm","740"]
["","","","Szerokość","mm","884"]
["","","","Głębokość","mm","388"]
["Ciężar","Jednostka","","","kg","58.5"]
["Zakres pracy","Chłodzenie","","Min.","°CDB","10"]
["","","","Maks.","°CDB","43"]
["","Ciepła woda użytkowa","","Min.","°CDB","-25"]
["","Ciepła woda użytk.","","Maks.","°CDB","35"]
["Poziom mocy akustycznej","Grzanie","","Nom.","dBA","60 (1)"]
["","Chłodzenie","","Nom.","dBA","62 (1)"]
["Poziom ciśnienia akustycznego","Grzanie","","Nom.","dBA","47 (1)"]
["","Chłodzenie","","Nom.","dBA","49 (1)"]
["Czynnik chłodniczy","Typ","","","","R-32"]
["","GWP","","","","675.0"]
["","Ilość","","","tCO2Eq","1.01"]
["","Ilość","","","kg","1.50"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6"]
["","Gaz","","Śr. zewn.","mm","15.9"]
["Połączenia instalacji","Spust","","Śr. zew.","mm","18"]
["","Różnica poziomów","IU - OU","Maks.","m","30.0"]
["Połączenia instalacji rurowej","Izolacja cieplna","","","","Rury z cieczą i gazem"]
["Zasilanie energią elektryczną","Nazwa","","","","V3"]
["","liczba faz","","","","1N~"]
["Zasilanie","Częstotliwość","","","Hz","50"]
["","Napięcie","","","V","230"]
["Prąd","zalecane bezpieczniki","","","A","20"]
["Uwagi","","","","","(1) - Ta chłodzenia 35°C - LWE 18° (DT = 5°C) – Ta grzania DB/WB 7°C/6°C - LWC 35° (DT = 5°C)"]