{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSH12E"]
[]
[]
[]
[]
["","","","","","ETSH12P30EF","ETSH12P50EF","ETSH12P50EG","ETSH12P30EG"]
["Obudowa","Kolor","","","","Biały (RAL9016) / Czarny (RAL9017)","Biały (RAL9016) / Czarny (RAL9017)","Biały (RAL9016) / Czarny (RAL9017)","Biały (RAL9016) / Czarny (RAL9017)"]
["","Materiał","","","","Polipropylen odporny na uderzenia","Polipropylen odporny na uderzenia","Polipropylen odporny na uderzenia","Polipropylen odporny na uderzenia"]
["Wymiary","Jednostka","","Wysokość","mm","1,892","1,910","1,910","1,891"]
["","","","Szerokość","mm","594","792","792","594"]
["","","","Głębokość","mm","644","816","817","644"]
["Ciężar","Jednostka","","","kg","75","98","98","75"]
["Poziom mocy akustycznej","Nom.","","","dBA","47.3","47.3","47.3","47.3"]
["Poziom ciśnienia akustycznego","Nom.","","","dBA","38.6","38.6","38.6","38.6"]
["Zakres pracy","Grzanie","Strona wodna","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Maks.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","Chłodzenie","Temp. otoczenia","Min.","°CDB","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","Strona wodna","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Maks.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50","50"]
["","Napięcie","","","V","230","230","230","230"]
["Uwagi","","","","","(1) - Straty ciepła według EN12897","(1) - Straty ciepła według EN12897","(1) - Straty ciepła według EN12897","(1) - Straty ciepła według EN12897"]
["","","","","","(2) - Zapoznać się z rysunkami limitów eksploatacyjnych","(2) - Zapoznać się z rysunkami limitów eksploatacyjnych","(2) - Zapoznać się z rysunkami limitów eksploatacyjnych","(2) - Zapoznać się z rysunkami limitów eksploatacyjnych"]