{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSXB-D"]
[]
[]
[]
[]
["","","","","","ETSXB16P30DA","ETSXB16P50DA"]
["Poziom ciśnienia akustycznego","Nom.","","","dBA","32.8","32.8"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","10","10"]
["","","Strona wodna","Maks.","°C","22","22"]
["","","","Min.","°C","5","5"]
["","Grzanie","Strona wodna","Maks.","°C","70","70"]
["","","","Min.","°C","15","15"]
["Sound power level","Nom.","","","dBA","45.6","45.6"]
["Wymiary","Jednostka","","Szerokość","mm","590","785"]
["","","","Głębokość","mm","615","785"]
["","","","Wysokość","mm","1,891","1,896"]
["Obudowa","Materiał","","","","Polipropylen odporny na uderzenia","Polipropylen odporny na uderzenia"]
["","Kolor","","","","Biały (RAL9016) / Ciemno-szary (RAL7011)","Biały (RAL9016) / Ciemno-szary (RAL7011)"]
["PED","Kategoria","","","","Art. 4.3","Art. 4.3"]
["Ciężar","Jednostka","","","kg","75","96"]
["Power supply","liczba faz","","","","1~","1~"]
["","Częstotliwość","","","Hz","50","50"]
["","Napięcie","","","V","230","230"]
["Grzałka elektryczna","Zasilanie","","Częstotliwość","Hz","50","50"]
["","","","Nazwa","","3V / 9W","3V / 9W"]
["","","","Faza","","1~ / 3~","1~ / 3~"]
["Uwagi","","","","","(1) - Straty ciepła według EN12897","(1) - Straty ciepła według EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]