{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":10,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWLQ-KC"]
[]
[]
[]
[]
["","","","","","EWLQ014KCW1N","EWLQ025KCW1N","EWLQ033KCW1N","EWLQ049KCW1N","EWLQ064KCW1N"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","55.2","55.2","62.1","57.6","64.6"]
["Czynnik chłodniczy","Obwody","","Ilość","","1","1","1","2","2"]
["","GWP","","","","2,088.0","2,088.0","2,088.0","2,088.0","2,088.0"]
["","Dopełnienie","","","kg","0.0","0.0","0.0","0.0","0.0"]
["","Typ","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Zakres pracy","Parownik","Chłodzenie","Min.","°CDB","-10","-10","-10","-10","-10"]
["","","","Maks.","°CDB","20","20","20","20","20"]
["Wydajność chłodnicza","Nom.","","","kW","12.09","19.87","28.90","39.35","57.84"]
["Power input","Chłodzenie","","Nom.","kW","3.74","6.11","8.43","12.03","16.41"]
["Sound power level","Chłodzenie","","Nom.","dBA","69.0","69.0","76.0","72.0","79.0"]
["Sprężarka","Typ","","","","Sprężarka spiralna","Sprężarka spiralna","Sprężarka spiralna","Sprężarka spiralna","Sprężarka spiralna"]
["","Ilość_","","","","1","1","1","2","2"]
["Wymiary","Jednostka","","Szerokość","mm","600","600","600","600","600"]
["","","","Głębokość","mm","600","600","600","1,200","1,200"]
["","","","Wysokość","mm","600","600","600","600","600"]
["Regulator wydajności","Minimalna wydajność","","","%","100","100","100","50","50"]
["","Metoda","","","","Stała","Stała","Stała","Stała","Stała"]
["Ciężar","Ciężar operacyjny","","","kg","70","129","135","247","258"]
["","Jednostka","","","kg","62","124","130","238","249"]
["Wodny wymiennik ciepła - parownik","Typ","","","","Płyta lutowana","Płyta lutowana","Płyta lutowana","Płyta lutowana","Płyta lutowana"]
["","Objętość wody","","","l","1.47","1.96","2.74","4.47","5.88"]
["EER","","","","","3.237","3.254","3.429","3.27","3.524"]
["Power supply","liczba faz","","","","3N~","3N~","3N~","3N~","3N~"]
["","Częstotliwość","","","Hz","50","50","50","50","50"]
["","Napięcie","","","V","400","400","400","400","400"]