{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Obudowa","Kolor","","","","Biały","Biały"]
["","Materiał","","","","Żywica","Żywica"]
["Wymiary","Jednostka","","Wysokość","mm","290","340"]
["","","","Szerokość","mm","1050","1200"]
["","","","Głębokość","mm","269","262"]
["Ciężar","Jednostka","","","kg","14","18"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","16.2","23"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","13.4","21.1"]
["","","","Niski","m³/min","12.1","18.7"]
["","","Grzanie","Wysoki","m³/min","16.9","23"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","14.2","20.9"]
["","","Grzanie","Niski","m³/min","12.7","18.7"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","61","65"]
["","Ogrzewanie","","","dBA","61","65"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","45","49"]
["","","","Czynnik","dBA","42","45"]
["","","","Niski","dBA","40","41"]
["","Grzanie","","Wysoki","dBA","45","49"]
["","Ogrzewanie","","Czynnik","dBA","42","45"]
["","Grzanie","","Niski","dBA","40","41"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","9.52","9.52"]
["","Gaz","","Śr. zewn.","mm","15.9","15.9"]
["","Spust","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50"]
["","Napięcie","","","V","220-240","220-240"]
["Standardowe akcesoria","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Uwagi","","","","","(1) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["Standardowe akcesoria","Screw cover","","","","","3"]