{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9 / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FAQ100CVEB9 / RZQG71L9V1B","FAQ71CVEB9 / RZQG71L9V1B","FAQ71CVEB9 / FAQ71CVEB9 / RZQG100L9V1B","FAQ100CVEB9 / RZQG100L9V1B","FAQ71CVEB9 / FAQ71CVEB9 / RZQG125L9V1B"]
["Wydajność chłodnicza","Nom.","","kW","","6.8","","9.5"]
["Chłodzenie pomieszczeń","SEER","","","6.51","6.43","5.10","6.11","5.10"]
["","Roczne zużycie energii","","kWh/rok","366","371","652","545","824"]
["","Wydajność","Pdesign","kW","6.80","6.80","9.50","9.50","12.00"]
["","Klasa efektywności energetycznej","","","A++","A++","B","A++","B"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Wydajność","Pdesign","kW","6.33","6.33","11.30","10.20","12.71"]
["","SCOP/A","","","4.02","4.02","3.80","4.01","3.80"]
["","Klasa efektywności energetycznej","","","A+","A+","A","A+","A"]
["","Roczne zużycie energii","","kWh/rok","2,205","2,205","4,164","3,562","4,683"]
["Efektywność nominalna","Annual energy consumption","","kWh","","1,000","","1,315"]
["","EER","","","","3.40","","3.62"]
["","COP","","","","3.70","","3.61"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","","A","","A"]
["","","Ogrzewanie","","","A","","A"]
["Wydajność grzewcza","Nom.","","kW","","7.5","","10.8"]
["Uwagi","","","","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską"]
["","","","","","(1) - Roczne zużycie energii jest zgodne z Dyrektywą na temat oznaczeń konsumpcji energii 2002/31/WE","","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską"]
["","","","","","(2) - Współczynniki SEER i SCOP zgodne z EN 14825","","(2) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)"]