{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9"]
[]
[]
[]
[]
["","","","","FAQ71CVEB9","FAQ100CVEB9"]
["Poziom ciśnienia akustycznego","Grzanie","Wysoki","dBA","45","49"]
["","","Nom.","dBA","42","45"]
["","","Czynnik","dBA","42","45"]
["","","Niski","dBA","40","41"]
["","Chłodzenie","Medium","dBA","42","45"]
["","","Niski","dBA","40","41"]
["","","Wysoki","dBA","45","49"]
["","","Nom.","dBA","42","45"]
["Wydajność chłodnicza","Całkowita wydajność","Nom.","kW","0.051","0.061"]
["Połączenia instalacji rurowej","Ciecz","Śr. zewn.","mm","9.52","9.52"]
["","Gaz","Śr. zewn.","mm","15.9","15.9"]
["","Spust","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Sound power level","Chłodzenie","","dBA","61","65"]
["","Ogrzewanie","","dBA","61","65"]
["Wymiary","Jednostka","Szerokość","mm","1,050","1,200"]
["","","Głębokość","mm","238","240"]
["","","Wysokość","mm","290","340"]
["Obudowa","Materiał","","","Żywica","Żywica"]
["","Kolor","","","Świeży biały","Świeży biały"]
["Ciężar","Jednostka","","kg","13","17"]
["Wydajność grzewcza","Wydajność całkowita","Nom.","kW","0.068","0.061"]
["Power supply","liczba faz","","","1~","1~"]
["","Częstotliwość","","Hz","50","50"]
["","Napięcie","","V","220-240","220-240"]