{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / 4MXM-N"]
[]
[]
[]
[]
["","","","","FBA35A2VEB9 / FBA35A2VEB9 / 4MXM68N2V1B"]
["Wydajność chłodnicza","Nom.","","kW","6.8"]
["Chłodzenie pomieszczeń","SEER","","","5.26"]
["","Roczne zużycie energii","","kWh/rok","453"]
["","Wydajność","Pdesign","kW","6.80"]
["","Klasa efektywności energetycznej","","","A"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Wydajność","Pdesign","kW","3.60"]
["","SCOP/A","","","3.81"]
["","Klasa efektywności energetycznej","","","A"]
["","Roczne zużycie energii","","kWh/rok","1,323"]
["Efektywność nominalna","Rocz. zużycie ener.","","kWh","1,245"]
["","EER","","","2.73"]
["","COP","","","3.24"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","D"]
["","","Ogrzewanie","","C"]
["Wydajność grzewcza","Nom.","","kW","8.60"]
["Uwagi","","","","(1) - Nominalne wydajności chłodzenia oparte są na: temperatura wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["","","","","(3) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","(4) - Dane elektryczne, patrz oddzielny rysunek"]