{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RZQ-C"]
[]
[]
[]
[]
["","","","","FBA50A2VEB9 / FBA50A2VEB9 / FBA50A2VEB9 / FBA50A2VEB9 / RZQ200C7Y1B","FBA60A2VEB9 / FBA60A2VEB9 / FBA60A2VEB9 / FBA60A2VEB9 / RZQ250C7Y1B"]
["Wydajność chłodnicza","Nom.","","kW","20.0 (1)"]
["Chłodzenie pomieszczeń","SEER","","","5.67"]
["","Roczne zużycie energii","","kWh/rok","2,115"]
["","Wydajność","Pdesign","kW","20.0"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Wydajność","Pdesign","kW","11.2"]
["","SCOP/A","","","3.68"]
["","Roczne zużycie energii","","kWh/rok","4,257"]
["Wydajność grzewcza","Nom.","","kW","23.0 (2)"]
["Uwagi","","","","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 7,5m; różnica poziomów: 0 m","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 7,5m; różnica poziomów: 0 m"]
["","","","","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m; różnica poziomów: 0 m","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m; różnica poziomów: 0 m"]
["","","","","(3) - Wartości te nie obejmują obniżenia wydajności przez operację odszraniania.","(3) - Wartości te nie obejmują obniżenia wydajności przez operację odszraniania."]
["Wydajność chłodnicza","Nom.","","kW","","24.1 (1)"]
["Wydajność grzewcza","Nom.","","kW","","26.4 (2)"]
["Chłodzenie pomieszczeń","Wydajność","Pdesign","kW","","24.1"]
["","SEER","","","","5.74"]
["","Roczne zużycie energii","","kWh/rok","","2518"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Wydajność","Pdesign","kW","","12.1"]
["","SCOP/A","","","","3.76"]
["","Roczne zużycie energii","","kWh/rok","","4484"]
["Zakres efektywności energetycznej","","","","","A+++ ~ D"]