{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RXL-K"]
[]
[]
[]
[]
["","","","","FBQ35C8VEB / RXL35K2V1B","FBQ50C8VEB / RXL50K2V1B"]
["Wydajność chłodnicza","Min.","","kW","1.4","1.7"]
["","Maks.","","kW","3.9","5.3"]
["","Nom.","","kW","3.40","5.00"]
["Efektywność nominalna","Annual energy consumption","","kWh","530","825"]
["","EER","","","3.21","3.03"]
["","COP","","","3.51","3.42"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A","B"]
["","","Ogrzewanie","","B","B"]
["Wydajność grzewcza","Nom.","","kW","4.00","5.50"]
["","Min.","","kW","1.3","1.6"]
["","Maks.","","kW","5.0","6.1"]
["Uwagi","","","","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską"]
["","","","","(2) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)","(2) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)"]