{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":7,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RXS-L"]
[]
[]
[]
[]
["","","","","FBQ35C8VEB / RXS35L2V1B","FBQ50C8VEB / RXS50L2V1B","FBQ60C8VEB / RXS60L2V1B"]
["Wydajność chłodnicza","Min.","","kW","1.4","1.7","1.7"]
["","Maks.","","kW","3.9","5.3","6.5"]
["","Nom.","","kW","3.40","5.0","5.7"]
["Połączenia instalacji rurowej","Ciecz","Śr. zewn.","mm","6.35","6.35","6.35"]
["","Gaz","Śr. zewn.","mm","9.5","12.7","12.7"]
["","Spust","Śr. zew.","mm","VP25 (Średnica zewnętrzna 32, średnica wewnętrzna 25)","VP25 (Średnica zewnętrzna 32, średnica wewnętrzna 25)","VP25 (Średnica zewnętrzna 32, średnica wewnętrzna 25)"]
["Efektywność nominalna","Rocz. zużycie ener.","","kWh","530","825","875"]
["","EER","","","3.21","3.03","3.26"]
["","COP","","","3.60","3.42","3.41"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A","B","A"]
["","","Ogrzewanie","","A","B","B"]
["Wydajność grzewcza","Nom.","","kW","4.00","5.5","7.0"]
["","Min.","","kW","1.3","1.7","1.7"]
["","Maks.","","kW","5.0","6.0","8.0"]
["Uwagi","","","","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską"]
["","","","","(2) - 220 V","(2) - 230 V","(2) - 230 V"]
["","","","","(3) - 230 V","(3) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)","(3) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)"]
["","","","","(4) - 240 V"]
["","","","","(5) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)"]