{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D / RXS-L"]
[]
[]
[]
[]
["","","","","FBQ50D2VEB / RXS50L2V1B","FBQ60D2VEB / RXS60L2V1B (Archived)"]
["Wydajność chłodnicza","Nom.","","kW","5.0 (2)"]
["Efektywność nominalna","Rocz. zużycie ener.","","kWh","710"]
["","EER","","","3.52 (1)"]
["","COP","","","3.83 (1)"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A"]
["","","Ogrzewanie","","A"]
["Wydajność grzewcza","Nom.","","kW","5.50 (2)"]
["Uwagi","","","","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską"]
["","","","","(2) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)","(2) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)"]
["Jednostka zewnętrzna","","","","","RXS60L"]
["Wydajność chłodnicza","Nom.","","kW","","5.7"]
["Wydajność grzewcza","Nom.","","kW","","7.00"]
["Wydaj. znam.","EER","","","","3.45"]
["","COP","","","","3.71"]
["","Rocz. zużycie ener.","","kWh","","826"]
["Efektywność nominalna","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","","A"]
["","","Ogrzewanie","","","A"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","","A+"]
["","Wydajność","Pdesign","kW","","5.70"]
["","SEER","","","","5.86"]
["","Roczne zużycie energii","","kWh/rok","","340"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","","A+"]
["","Wydajność","Pdesign","kW","","4.60"]
["","SCOP/A","","","","4.01"]
["","Roczne zużycie energii","","kWh/rok","","1606"]