{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":12,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D"]
[]
[]
[]
[]
["","","","","","FBQ35D2VEB","FBQ50D2VEB","FBQ60D2VEB","FBQ71D2VEB","FBQ100D2VEB","FBQ125D2VEB","FBQ140D2VEB"]
["Poziom ciśnienia akustycznego","Grzanie","","Wysoki","dBA","37","37","31","31.0","36.0","38.0","38"]
["","","","Czynnik","dBA","34","34","28","28.0","33.0","35.0","35"]
["","","","Niski","dBA","29","29","25","25.0","30.0","32.0","32"]
["","Chłodzenie","","Medium","dBA","32","32","28","28.0","32.0","35.0","35"]
["","","","Niski","dBA","29","29","25","25.0","30.0","32.0","32"]
["","","","Wysoki","dBA","35","35","30","30.0","34.0","37.0","37"]
["Standardowe akcesoria","Instrukcja obsługi","","","","1","1","1","1","1","1","1"]
["","Instrukcja instalacji","","","","1","1","1","1","1","1","1"]
["","Przewód spustowy","","","","1","1","1","1","1","1","1"]
["","Zacisk metalowy na przewodzie spustowym","","","","1","1","1","1","1","1","1"]
["","Podkładka do wspornika wieszaka","","","","8","8","8","8","8","8","8"]
["","Śruby","","","","40","40","40","40","40","40","40"]
["","Izolacja mocowania","","","","2","2","2","2","2","2","2"]
["","Podkładka uszczelniająca","","","","5","5","5","5","5","5","5"]
["","Podkładki uszczelniające","","","","","","","5","5","5","5"]
["","Zaciski","","","","4","4","4","4","4","4","4"]
["Czynnik chłodniczy","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["Control systems","Wired remote control","","","","","","","BRC1E52A/B, BRC1D528","BRC1E52A/B, BRC1D528","BRC1E52A/B, BRC1D528","BRC1E52A/B, BRC1D528"]
["","Infrared remote control","","","","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Gaz","","Śr. zewn.","mm","9.52","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Spust","","","","VP20 (śr. wew. 20/śr. zew. 26), wysokość spustu 625 mm","VP20 (śr. wew. 20/śr. zew. 26), wysokość spustu 625 mm","VP20 (śr. wew. 20/śr. zew. 26), wysokość spustu 625 mm","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Chłodzenie","","","dBA","60","60","56","56","58","62","62"]
["Wymiary","Jednostka","","Szerokość","mm","700","700","1,000","1,000","1,400","1,400","1,400"]
["","","","Głębokość","mm","800","800","800","800","800","800","800"]
["","","","Wysokość","mm","245","245","245","245","245","245","245"]
["Obudowa","Materiał","","","","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa"]
["","Kolor","","","","Nie pokryta (galwanizowana)","Nie pokryta (galwanizowana)","Nie pokryta (galwanizowana)","Nie pokryta (galwanizowana)","Nie pokryta (galwanizowana)","Nie pokryta (galwanizowana)","Nie pokryta (galwanizowana)"]
["Ciężar","Jednostka","","","kg","28.0","28.0","35.0","35.0","46.0","46.0","46.0"]
["Wentylator","Spręż dyspozycyjny","","Wysoki","Pa","150","150","150","150","150","150","150"]
["","","","Nom.","Pa","30","30","30","30","40","50","50"]
["","Przepływ powietrza","Grzanie","Wysoki","m³/min","","","","","29.0","34.0","34.0"]
["","","","Niski","m³/min","","","","","23.0","23.5","23.5"]
["","","","Medium","m³/min","","","","","26.0","29.0","29.0"]
["","","Chłodzenie","Niski","m³/min","","","","","23.0","23.5","23.5"]
["","","","Medium","m³/min","","","","","26.0","29.0","29.0"]
["","","","Wysoki","m³/min","","","","","29.0","34.0","34.0"]
["Wysokość spustu","mm","","","","625","625","625","625","625","625","625"]
["Power supply","liczba faz","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Częstotliwość","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Nazwa","","","","VE","VE","VE","VE","VE","VE","VE"]
["","Napięcie","","","V","220-240","220-240","220-240","220-240/220","220-240/220","220-240/220","220-240/220"]
["Uwagi","","","","","(1) - Poziom mocy akustycznej to warto absolutna oznaczająca moc wytwarzaną przez źródło dźwięku.","(1) - Poziom mocy akustycznej to warto absolutna oznaczająca moc wytwarzaną przez źródło dźwięku.","(1) - Poziom mocy akustycznej to warto absolutna oznaczająca moc wytwarzaną przez źródło dźwięku.","(1) - Poziom mocy akustycznej to warto absolutna oznaczająca moc wytwarzaną przez źródło dźwięku.","(1) - Poziom mocy akustycznej to warto absolutna oznaczająca moc wytwarzaną przez źródło dźwięku.","(1) - Poziom mocy akustycznej to warto absolutna oznaczająca moc wytwarzaną przez źródło dźwięku.","(1) - Poziom mocy akustycznej to warto absolutna oznaczająca moc wytwarzaną przez źródło dźwięku."]