{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":7,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / AZAS-MY"]
[]
[]
[]
[]
["","","","","FCAG100BVEB / AZAS100MUY","FCAG125BVEB / AZAS125MUY","FCAG140BVEB / AZAS140MUY"]
["Wydajność chłodnicza","Nom.","","kW","9.50 (1)","12.1 (1)","13.4 (1)"]
["Wydajność grzewcza","Nom.","","kW","10.8 (2)","13.5 (2)","15.5 (2)"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","A++"]
["","Wydajność","Pdesign","kW","9.50","12.1","13.4"]
["","SEER","","","6.12","5.62","6.20"]
["","Roczne zużycie energii","","kWh/rok","543","1292","1296"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","A"]
["","Wydajność","Pdesign","kW","6.00","6.00","7.80"]
["","SCOP/A","","","3.85","3.80","4.31"]
["","Roczne zużycie energii","","kWh/rok","2182","2211","2534"]
["Zakres efektywności energetycznej","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Uwagi","","","","(1) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m.","(1) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m.","(1) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m.","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m.","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["","","","","(3) - Patrz oddzielny rysunek zakresu pracy","(3) - Patrz oddzielny rysunek zakresu pracy","(3) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","(4) - Dane elektryczne, patrz oddzielny rysunek","(4) - Dane elektryczne, patrz oddzielny rysunek","(4) - Dane elektryczne, patrz oddzielny rysunek"]