{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":8,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","FCAG71BVEB / AZQS71B2V1B","FCAG100BVEB / AZQS100B8V1B","FCAG125BVEB / AZQS125B8V1B","FCAG140BVEB / AZQS140B8V1B"]
["Wydajność chłodnicza","Nom.","","kW","6.8 (1)","9.5 (1)","12.1 (1)","13.0 (1)"]
["Wydajność grzewcza","Nom.","","kW","7.5 (2)","10.8 (2)","13.5 (2)","15.5 (2)"]
["Efektywność nominalna","EER","","","3.11 (3)","3.21 (3)","2.22 (3)","2.63 (3)"]
["","COP","","","3.61 (3)","3.50 (3)","3.41 (3)","3.30 (3)"]
["","Rocz. zużycie ener.","","kWh","1,093","1,480"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","B","A"]
["","","Ogrzewanie","","A","B"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","A+","A"]
["","Wydajność","Pdesign","kW","6.8","9.5","12.1","13.0"]
["","SEER","","","5.70","5.50","5.16","5.94"]
["","Roczne zużycie energii","","kWh/rok","418","605","1,406","1,314"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","A+","A"]
["","Wydajność","Pdesign","kW","6.3","7.6","7.8","11.6"]
["","SCOP/A","","","4.00","3.85","3.67","3.96"]
["","Roczne zużycie energii","","kWh/rok","2,216","2,762","2,969","4,089"]
["Uwagi","","","","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 7,5m; różnica poziomów: 0 m","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 7,5m; różnica poziomów: 0 m","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 7,5m; różnica poziomów: 0 m","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 7,5m; różnica poziomów: 0 m"]
["","","","","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m; różnica poziomów: 0 m","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m; różnica poziomów: 0 m","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m; różnica poziomów: 0 m","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m; różnica poziomów: 0 m"]
["","","","","(3) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(3) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(3) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(3) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską"]