{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":23,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100BVEB / RZQG100L8Y1B","FCAG125BVEB / RZQG125L8Y1B","FCAG140BVEB / RZQG100L8Y1B","FCAG140BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG60BVEB / FCAG60BVEB / RZQG125L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG100L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG71L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG71BVEB / RZQG71L8Y1B","FCAG100BVEB / RZQG71L8Y1B","FCAG140BVEB / RZQG140L7Y1B"]
["Zakres efektywności energetycznej","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Wydajność chłodnicza","Nom.","","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["Efektywność nominalna","EER","","","","","","","","","","","","","","","","3.30","3.30","3.30","3.39","3.39","2.50"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","","","","","","","","","","","","","","A","A","A","A++","A++"]
["","Wydajność","Pdesign","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["","SEER","","","","","","","","","","","","","","","","5.10","5.10","5.10","6.72","6.80","6.44"]
["","Roczne zużycie energii","","kWh/rok","","","","","","","","","","","","","","467","467","467","355","350","1,249"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","","","","","","","","","","","","","","A","A","A","A+","A+"]
["","Wydajność","Pdesign","kW","","","","","","","","","","","","","","6.00","6.00","6.00","6.33","6.33","11.56"]
["","SCOP/A","","","","","","","","","","","","","","","","3.80","3.80","3.80","4.20","4.20","4.27"]
["","Roczne zużycie energii","","kWh/rok","","","","","","","","","","","","","","2,211","2,211","2,211","2,110","2,110","3,795"]
["Uwagi","","","","","","","","","","","","","","","","","(1) - Nominalne wydajności chłodzenia oparte są na: temperatura wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m.","(1) - Patrz oddzielny rysunek zakresu pracy","(1) - Patrz oddzielny rysunek zakresu pracy","(1) - Nominalne wydajności chłodzenia oparte są na: temperatura wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m.","(1) - Patrz oddzielny rysunek zakresu pracy","(1) - Nominalne wydajności chłodzenia oparte są na: temperatura wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","","","","","","","","","","","","","","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m.","(2) - Dane elektryczne, patrz oddzielny rysunek","(2) - Dane elektryczne, patrz oddzielny rysunek","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m.","(2) - Dane elektryczne, patrz oddzielny rysunek","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["","","","","","","","","","","","","","","","","","(3) - Patrz oddzielny rysunek zakresu pracy","","","(3) - Patrz oddzielny rysunek zakresu pracy","","(3) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","","","","","","","","","","","","","","(4) - Dane elektryczne, patrz oddzielny rysunek","","","(4) - Dane elektryczne, patrz oddzielny rysunek","","(4) - Dane elektryczne, patrz oddzielny rysunek"]
["Wydajność grzewcza","Nom.","","kW","","","","","","","","","","","","","","","","","7.50","","15.50"]
["Efektywność nominalna","COP","","","","","","","","","","","","","","","","","","","3.97","","3.61"]
["","Rocz. zużycie ener.","","kWh","","","","","","","","","","","","","","","","","1,003"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","","","","","","","","","","","","","","","","","A"]
["","","Ogrzewanie","","","","","","","","","","","","","","","","","","A"]