{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":61,"n_cols":12,"rows_kept":61,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B"]
[]
[]
[]
[]
["","","","","","FCAG35BVEB","FCAG50BVEB","FCAG60BVEB","FCAG71BVEB","FCAG100BVEB","FCAG125BVEB","FCAG140BVEB"]
["Wydajność chłodnicza","Całkowita wydajność","","Nom.","kW","3.50","5.00","5.70","6.80","9.50","12.10","13.40"]
["Wydajność grzewcza","Wydajność całkowita","","Nom.","kW","4.2","6.0","7.0","7.5","10.8","13.5","15.5"]
["Obudowa","Materiał","","","","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa"]
["Wymiary","Jednostka","","Wysokość","mm","204","204","204","204","246","246","246"]
["","","","Szerokość","mm","840","840","840","840","840","840","840"]
["","","","Głębokość","mm","840","840","840","840","840","840","840"]
["Ciężar","Jednostka","","","kg","18","19","19","21","23","23","23"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","12.9","14.6","14.9","15.1","22.7","27.2","27.2"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","10.6","11.8","12.2","13","17.8","20.4","20.4"]
["","","","Niski","m³/min","8.8","9.4","9.6","10.8","13","13.1","13.1"]
["","","Grzanie","Wysoki","m³/min","14.1","14.6","14.9","15.1","23","27","27"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","11.6","11.8","12.2","12.9","18.1","20.2","20.2"]
["","","Grzanie","Niski","m³/min","9.4","9.4","9.6","10.8","13.2","13","13"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","49","49","51","51","54","58","58"]
["","Ogrzewanie","","","dBA","49","49","51","51","54","58","58"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","31","31","33","35","37","41","41"]
["","","","Czynnik","dBA","29","29","31","31","33","35","35"]
["","","","Niski","dBA","27","27","28","28","29","29","29"]
["","Grzanie","","Wysoki","dBA","31","31","33","33","37","41","41"]
["","Ogrzewanie","","Czynnik","dBA","29","29","31","31","33","35","35"]
["","Grzanie","","Niski","dBA","27","27","28","28","29","29","29"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Gaz","","Śr. zewn.","mm","9.52","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Spust","","","","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)"]
["Panel dekoracyjny","Model","","","","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B"]
["","Wymiary","","Wysokość","mm","65","65","65","65","65","65","65"]
["","","","Szerokość","mm","950","950","950","950","950","950","950"]
["","","","Głębokość","mm","950","950","950","950","950","950","950"]
["","Ciężar","","","kg","5.5","5.5","5.5","5.5","5.5","5.5","5.5"]
["Panel dekoracyjny 2","Model","","","","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B"]
["","Wymiary","","Wysokość","mm","148","148","148","148","148","148","148"]
["","","","Szerokość","mm","950","950","950","950","950","950","950"]
["","","","Głębokość","mm","950","950","950","950","950","950","950"]
["","Ciężar","","","kg","10.3","10.3","10.3","10.3","10.3","10.3","10.3"]
["Panel dekoracyjny 3","Model","","","","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB"]
["","Wymiary","","Wysokość","mm","106","106","106","106","106","106","106"]
["","","","Szerokość","mm","950","950","950","950","950","950","950"]
["","","","Głębokość","mm","950","950","950","950","950","950","950"]
["","Ciężar","","","kg","6.5","6.5","6.5","6.5","6.5","6.5","6.5"]
["Syst. kontroli","Pilot na podczerwień","","","","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB"]
["","Pilot przewodowy","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7"]
["Standardowe akcesoria","Installation manual","","","","1","1","1","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8","8","8","8"]
["","Operation manual","","","","1","1","1","1","1","1","1"]
["","Wire clamp material","","","","7","7","7","7","7","7","7"]
["","Clamp for drain hose","","","","1","1","1","1","1","1","1"]
["","Clamps","","","","1","1","1","1","1","1","1"]
["","Drain hose","","","","1","1","1","1","1","1","1"]
["","Installation guide","","","","1","1","1","1","1","1","1"]
["","Insulation for fitting","","","","2","2","2","2","2","2","2"]
["","Screws","","","","4","4","4","4","4","4","4"]
["","Sealing pads","","","","1","1","1","1","1","1","1"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~","1~","1~","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Napięcie","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]