{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":13,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZQG100L8Y1B","FCAHG125GVEB / RZQG125L8Y1B","FCAHG100GVEB / RZQG71L8Y1B","FCAHG71GVEB / RZQG71L8Y1B","FCAHG140GVEB / RZQG100L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG100L8Y1B","FCAHG140GVEB / RZQG125L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG140L7Y1B"]
["Wydajność chłodnicza","Nom.","","kW","","","","6.80 (1)","","","","","13.4 (1)"]
["Chłodzenie pomieszczeń","SEER","","","","","6.91","6.91","","","","","6.75"]
["","ηs,c","","%","","","","","","","","","266.9"]
["","Roczne zużycie energii","","kWh/rok","","","345","345","","","","","1,191"]
["","Wydajność","Pdesign","kW","","","6.80","6.80","","","","","13.4"]
["","Klasa efektywności energetycznej","","","","","A++","A++"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Wydajność","Pdesign","kW","","","7.60","7.60","","","","","11.8"]
["","SCOP/A","","","","","4.54","4.54","","","","","4.38"]
["","Klasa efektywności energetycznej","","","","","A+","A+"]
["","Roczne zużycie energii","","kWh/rok","","","2,344","2,344","","","","","3,766"]
["","ηs,h","","%","","","","","","","","","172.1"]
["Efektywność nominalna","Annual energy consumption","","kWh","","","","830"]
["","EER","","","","","","4.09 (3)","","","","","3.18 (3)"]
["","COP","","","","","","4.80 (3)","","","","","4.12 (3)"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","","","","A"]
["","","Ogrzewanie","","","","","A"]
["Wydajność grzewcza","Nom.","","kW","","","","7.50 (2)","","","","","15.5 (2)"]
["Zakres efektywności energetycznej","","","","A+++ ~ D","A+++ ~ D","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Uwagi","","","","","","","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 7,5m; różnica poziomów: 0 m","","","","","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 7,5m; różnica poziomów: 0 m"]
["","","","","","","","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m; różnica poziomów: 0 m","","","","","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m; różnica poziomów: 0 m"]
["","","","","","","","(3) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","","","","","(3) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską"]
["Outdoor unit","","","","","","","","","RZQG100L8Y1","","RZQG125L8Y1"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","","","","","","A","","A"]
["","Wydajność","Pdesign","kW","","","","","","9.50","","12.0"]
["","SEER","","","","","","","","5.10","","5.10"]
["","Roczne zużycie energii","","kWh/rok","","","","","","652","","824"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","","","","","","A","","A"]
["","Wydajność","Pdesign","kW","","","","","","11.30","","12.71"]
["","SCOP/A","","","","","","","","3.80","","3.80"]
["","Pdh Wydajność grzewcza w temp. -10°","","kW","","","","","","9.66","","11.4"]
["","Roczne zużycie energii","","kWh/rok","","","","","","4164","","4683"]