{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZQSG100L8Y1B","FCAHG125GVEB / RZQSG125L8Y1B","FCAHG140GVEB / RZQSG140L7Y1B"]
["Wydajność chłodnicza","Nom.","","kW","9.50 (1)","12.0 (1)","13.4 (1)"]
["Chłodzenie pomieszczeń","Roczne zużycie energii","","kWh/rok","497","778"]
["","Wydajność","Pdesign","kW","9.50","12.0"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Wydajność","Pdesign","kW","8.03","8.03"]
["","Roczne zużycie energii","","kWh/rok","2,615","2,742"]
["Efektywność nominalna","Annual energy consumption","","kWh","1,285","1,855"]
["","EER","","","3.70 (3)","3.23 (3)","3.11 (3)"]
["","COP","","","4.30 (3)","3.75 (3)","3.61 (3)"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A","A"]
["","","Ogrzewanie","","A","A"]
["Wydajność grzewcza","Nom.","","kW","10.8 (2)","13.5 (2)","15.5 (2)"]
["Uwagi","","","","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 7,5m; różnica poziomów: 0 m","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 7,5m; różnica poziomów: 0 m","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 7,5m; różnica poziomów: 0 m"]
["","","","","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m; różnica poziomów: 0 m","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m; różnica poziomów: 0 m","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m; różnica poziomów: 0 m"]
["","","","","(3) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(3) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(3) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską"]
["Chłodzenie pomieszczeń","SEER","","","6.70","5.40"]
["","Klasa efektywności energetycznej","","","A++","A"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","SCOP/A","","","4.30","4.10"]
["","Klasa efektywności energetycznej","","","A+","A+"]