{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / AZQS-BY1 UK"]
[]
[]
[]
[]
["","","","","FCQG100FVEB / AZQS100B7Y1B UK","FCQG125FVEB / AZQS125B7Y1B UK","FCQG140FVEB / AZQS140B7Y1B UK"]
["Wydajność chłodnicza","Nom.","","kW","9.5","12.1","13.0"]
["Chłodzenie pomieszczeń","SEER","","","5.50"]
["","Roczne zużycie energii","","kWh/rok","605"]
["","Wydajność","Pdesign","kW","9.50"]
["","Klasa efektywności energetycznej","","","A"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Wydajność","Pdesign","kW","7.60"]
["","SCOP/A","","","3.85"]
["","Klasa efektywności energetycznej","","","A"]
["","Roczne zużycie energii","","kWh/rok","2,764"]
["Efektywność nominalna","Rocz. zużycie ener.","","kWh","1,480","1,952","2,313"]
["","EER","","","3.21","3.10","2.81"]
["","COP","","","3.50","3.41","3.30"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A","B"]
["","","Ogrzewanie","","B","B"]
["Wydajność grzewcza","Nom.","","kW","10.8","13.5","15.5"]
["Uwagi","","","","(1) - Roczne zużycie energii jest zgodne z Dyrektywą na temat oznaczeń konsumpcji energii 2002/31/WE","(1) - Roczne zużycie energii jest zgodne z Dyrektywą na temat oznaczeń konsumpcji energii 2002/31/WE","(1) - Roczne zużycie energii jest zgodne z Dyrektywą na temat oznaczeń konsumpcji energii 2002/31/WE"]
["","","","","(2) - Współczynniki SEER i SCOP zgodne z EN 14825","(2) - Współczynniki SEER i SCOP zgodne z EN 14825","(2) - Współczynniki SEER i SCOP zgodne z EN 14825"]
["","","","","(3) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)","(3) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)","(3) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)"]