{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RXS-L3"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / RXS35L3V1B"]
["Wydajność chłodnicza","Min.","","kW","1.3"]
["","Maks.","","kW","4.0"]
["","Nom.","","kW","3.4 (2)"]
["Połączenia instalacji rurowej","Ciecz","Śr. zewn.","mm","6.35"]
["","Gaz","Śr. zewn.","mm","9.5"]
["","Spust","Śr. zew.","mm","VP25 (Średnica zewnętrzna 32, średnica wewnętrzna 25)"]
["Efektywność nominalna","Rocz. zużycie ener.","","kWh","455"]
["","EER","","","3.74 (1)"]
["","COP","","","3.50 (1)"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A"]
["","","Ogrzewanie","","B"]
["Wydajność grzewcza","Nom.","","kW","4.20 (2)"]
["","Min.","","kW","1.3"]
["","Maks.","","kW","5.2"]
["Uwagi","","","","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską"]
["","","","","(2) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)"]
["","","","","(3) - 220 V"]
["","","","","(4) - 230 V"]
["","","","","(5) - 240 V"]