{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":117,"n_cols":9,"rows_kept":117,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F"]
[]
[]
[]
[]
["","","","","","FCQHG71FVEB","FCQHG100FVEB","FCQHG125FVEB","FCQHG140FVEB"]
["Poziom ciśnienia akustycznego","Grzanie","","Wysoki","dBA","","44","45","45"]
["","","","Nom.","dBA","","39","40","41"]
["","","","Niski","dBA","","33","35","37"]
["","Chłodzenie","","Niski","dBA","","33","35","37"]
["","","","Wysoki","dBA","","44","45","45"]
["","","","Nom.","dBA","","39","40","41"]
["Standardowe akcesoria","Instrukcja obsługi","","","","","Instrukcja obsługi","Instrukcja obsługi","Instrukcja obsługi"]
["","Instrukcja instalacji","","","","","Instrukcja instalacji","Instrukcja instalacji","Instrukcja instalacji"]
["","Przewód spustowy","","","","","Przewód spustowy","Przewód spustowy","Przewód spustowy"]
["","Zacisk przewodu spustowego","","","","","Zacisk przewodu spustowego","Zacisk przewodu spustowego","Zacisk przewodu spustowego"]
["","Podkładka do wspornika wieszaka","","","","","Podkładka do wspornika wieszaka","Podkładka do wspornika wieszaka","Podkładka do wspornika wieszaka"]
["","Śruby","","","","","Śruby","Śruby","Śruby"]
["","Przewodnik po instalacji","","","","","Przewodnik po instalacji","Przewodnik po instalacji","Przewodnik po instalacji"]
["","Izolacja mocowania","","","","","2","2","2"]
["","Podkładki uszczelniające","","","","","4","4","4"]
["","Podkładka uszczelniająca otworu spustowego","","","","","Podkładka uszczelniająca otworu spustowego","Podkładka uszczelniająca otworu spustowego","Podkładka uszczelniająca otworu spustowego"]
["","Zaciski","","","","","Zaciski","Zaciski","Zaciski"]
["Syst. kontroli","Pilot przewodowy","","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","","","BRC7FA532F","BRC7FA532F","BRC7FA532F"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","","9.52","9.52","9.52"]
["","Gaz","","Śr. zewn.","mm","","15.9","15.9","15.9"]
["","Spust","","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Panel dekoracyjny 4","Wymiary","","Głębokość","mm","","50","50","50"]
["","","","Szerokość","mm","","950","950","950"]
["","","","Wysokość","mm","","950","950","950"]
["","Model","","","","","BYCQ140D7W1 - z szarymi żaluzjami","BYCQ140D7W1 - z szarymi żaluzjami","BYCQ140D7W1 - z szarymi żaluzjami"]
["","Kolor","","","","","Biały (RAL 9010)","Biały (RAL 9010)","Biały (RAL 9010)"]
["","Ciężar","","","kg","","5.4","5.4","5.4"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","","61","61","61"]
["","Ogrzewanie","","","dBA","","61","61","61"]
["Wymiary","Jednostka","","Szerokość","mm","","840","840","840"]
["","","","Głębokość","mm","","840","840","840"]
["","","","Wysokość","mm","","288","288","288"]
["Obudowa","Materiał","","","","","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa"]
["Ciężar","Jednostka","","","kg","","26","26","26"]
["Panel dekoracyjny","Ciężar","","","kg","","10.3","10.3","10.3"]
["","Model","","","","","BYCQ140D7GFW1 - Panel z funkcja automatycznego czyszczenia, drobniejszą siatką filtracyjną","BYCQ140D7GFW1 - Panel z funkcja automatycznego czyszczenia, drobniejszą siatką filtracyjną","BYCQ140D7GFW1 - Panel z funkcja automatycznego czyszczenia, drobniejszą siatką filtracyjną"]
["","Wymiary","","Wysokość","mm","","130","130","130"]
["","","","Głębokość","mm","","950","950","950"]
["","","","Szerokość","mm","","950","950","950"]
["","Kolor","","","","","Czysto biały (RAL 9010)","Czysto biały (RAL 9010)","Czysto biały (RAL 9010)"]
["Power supply","liczba faz","","","","","1~","1~","1~"]
["","Częstotliwość","","","Hz","","50","50","50"]
["","Nazwa","","","","","VE","VE","VE"]
["","Napięcie","","","V","","220-240","220-240","220-240"]
["Uwagi","","","","","","(1) - Poziom mocy akustycznej to warto absolutna oznaczająca moc wytwarzaną przez źródło dźwięku.","(1) - Poziom mocy akustycznej to warto absolutna oznaczająca moc wytwarzaną przez źródło dźwięku.","(1) - Poziom mocy akustycznej to warto absolutna oznaczająca moc wytwarzaną przez źródło dźwięku."]
["","","","","","","(2) - BYCQ140D7W1W ma białą izolację. Należy pamiętać że osiadający brud jest bardziej widoczny na białej izolacji i dlatego zaleca się instalowanie panelu dekoracyjnego BYCQ140D7W1W w środowiskach zanieczyszczonych.","(2) - BYCQ140D7W1W ma białą izolację. Należy pamiętać że osiadający brud jest bardziej widoczny na białej izolacji i dlatego zaleca się instalowanie panelu dekoracyjnego BYCQ140D7W1W w środowiskach zanieczyszczonych.","(2) - BYCQ140D7W1W ma białą izolację. Należy pamiętać że osiadający brud jest bardziej widoczny na białej izolacji i dlatego zaleca się instalowanie panelu dekoracyjnego BYCQ140D7W1W w środowiskach zanieczyszczonych."]
["","","","","","","(3) - BYCQ140D7W1: biały panel standardowy z szarymi żaluzjami; BYCQ140D7W1W: biały panel standardowy z białymi żaluzjami; BYCQ140D7GW1: biały panel z funkcją automatycznego czyszczenia.","(3) - BYCQ140D7W1: biały panel standardowy z szarymi żaluzjami; BYCQ140D7W1W: biały panel standardowy z białymi żaluzjami; BYCQ140D7GW1: biały panel z funkcją automatycznego czyszczenia.","(3) - BYCQ140D7W1: biały panel standardowy z szarymi żaluzjami; BYCQ140D7W1W: biały panel standardowy z białymi żaluzjami; BYCQ140D7GW1: biały panel z funkcją automatycznego czyszczenia."]
["Obudowa","Materiał","","","","Galwanizowana blacha stalowa"]
["Wymiary","Jednostka","","Wysokość","mm","288"]
["","","","Szerokość","mm","840"]
["","","","Głębokość","mm","840"]
["Ciężar","Jednostka","","","kg","25"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","21.2"]
["","","","Nom.","m³/min","16.7"]
["","","","Niski","m³/min","12.2"]
["","","Grzanie","Wysoki","m³/min","21.2"]
["","","","Nom.","m³/min","16.7"]
["","","","Niski","m³/min","12.2"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","53"]
["","Ogrzewanie","","","dBA","53"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","36"]
["","","","Nom.","dBA","33"]
["","","","Niski","dBA","29"]
["","Grzanie","","Wysoki","dBA","36"]
["","","","Nom.","dBA","33"]
["","","","Niski","dBA","29"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","9.52"]
["","Gaz","","Śr. zewn.","mm","15.9"]
["","Spust","","","","VP25 (I.D. 25/O.D. 32)"]
["Panel dekoracyjny","Model","","","","BYCQ140D7GFW1 - Panel z funkcja automatycznego czyszczenia, drobniejszą siatką filtracyjną"]
["","Kolor","","","","Czysto biały (RAL 9010)"]
["","Wymiary","","Wysokość","mm","130"]
["","","","Szerokość","mm","950"]
["","","","Głębokość","mm","950"]
["","Ciężar","","","kg","10.3"]
["Panel dekoracyjny 2","Model","","","","BYCQ140D7GW1 - panel z funkcją automatycznego czyszczenia"]
["","Kolor","","","","Czysto biały (RAL 9010)"]
["","Wymiary","","Wysokość","mm","130"]
["","","","Szerokość","mm","950"]
["","","","Głębokość","mm","950"]
["","Ciężar","","","kg","10.3"]
["Panel dekoracyjny 3","Model","","","","BYCQ140D7W1W - cały biały"]
["","Kolor","","","","Czysto biały (RAL 9010)"]
["","Wymiary","","Wysokość","mm","50"]
["","","","Szerokość","mm","950"]
["","","","Głębokość","mm","950"]
["","Ciężar","","","kg","5.4"]
["Panel dekoracyjny 4","Model","","","","BYCQ140D7W1 - biały z szarymi żaluzjami"]
["","Kolor","","","","Czysto biały (RAL 9010)"]
["","Wymiary","","Wysokość","mm","950"]
["","","","Szerokość","mm","950"]
["","","","Głębokość","mm","50"]
["","Ciężar","","","kg","5.4"]
["Syst. kontroli","Infrared remote control","","","","BRC7FA532F"]
["Syst. kontroli","Pilot przewodowy","","","","BRC1D52, BRC1E52A/B"]
["Standardowe akcesoria","Installation manual","","","","Installation manual"]
["","Washer for hanger bracket","","","","Washer for hanger bracket"]
["","Operation manual","","","","Operation manual"]
["","Clamp for drain hose","","","","Clamp for drain hose"]
["","Clamps","","","","Clamps"]
["","Drain hose","","","","Drain hose"]
["","Drain sealing pad","","","","Drain sealing pad"]
["","Installation guide","","","","Installation guide"]
["","Insulation for fitting","","","","2"]
["","Screws","","","","Screws"]
["","Sealing pads","","","","4"]
["Zasilanie energią elektryczną","Nazwa","","","","VE"]
["","liczba faz","","","","1~"]
["Zasilanie","Zasilanie-=-Częstotliwość","","Częstotliwość","","50"]
["","Zasilanie-=-Napięcie","","Napięcie","","220-240"]