{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FDA125A5VEB / RZQSG125L9V1B"]
["Wydajność chłodnicza","Nom.","","kW","12.00"]
["Chłodzenie pomieszczeń","SEER","","","5.20"]
["","Roczne zużycie energii","","kWh/rok","808"]
["","Wydajność","Pdesign","kW","12.00"]
["","Klasa efektywności energetycznej","","","A"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Wydajność","Pdesign","kW","7.60"]
["","SCOP/A","","","3.90"]
["","Klasa efektywności energetycznej","","","A"]
["","Roczne zużycie energii","","kWh/rok","2,729"]
["Efektywność nominalna","Annual energy consumption","","kWh","1,942"]
["","EER","","","3.09"]
["","COP","","","3.51"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","B"]
["","","Ogrzewanie","","B"]
["Wydajność grzewcza","Nom.","","kW","13.50"]
["Uwagi","","","","(1) - Nominalne wydajności chłodzenia oparte są na: temperatura wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["","","","","(3) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","(4) - Dane elektryczne, patrz oddzielny rysunek"]