{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Wydajność chłodnicza","Całkowita wydajność","","Nom.","kW","12.10","19.00","22.00"]
["Wydajność grzewcza","Wydajność całkowita","","Nom.","kW","13.50","22.4","24.0"]
["Casing","Colour","","","","Nie powlekana","Nie powlekana","Nie powlekana"]
["","Material","","","","Stal galwanizowana","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa"]
["Wymiary","Jednostka","","Wysokość","mm","300","470","470"]
["","","","Szerokość","mm","1,400","1,490","1,490"]
["","","","Głębokość","mm","700","1,100","1,100"]
["Ciężar","Jednostka","","","kg","45","104","115"]
["Wymagana przestrzeń międzystropowa >","mm","","","","350"]
["Fan","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","39.0","64.0","69.0"]
["","","","Czynnik","m³/min","","50","56"]
["","","","Niski","m³/min","28.0","36.0","43.0"]
["","","Grzanie","Wysoki","m³/min","39.0","64.0","69.0"]
["","","","Czynnik","m³/min","","50.0","56.0"]
["","","","Niski","m³/min","28.0","36.0","43.0"]
["","Spręż dyspozycyjny","","Wysokie","Pa","200","250","250"]
["","","","Nom.","Pa","50","62","62"]
["Sound power level","Chłodzenie","","","dBA","66","69.0","71.0"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","40","43.0","44.0"]
["","","","Czynnik","dBA","","39.0","40.0"]
["","","","Niski","dBA","33","36.0","37.0"]
["","Grzanie","","Wysoki","dBA","40","43.0","44.0"]
["","","","Czynnik","dBA","","39.0","40.0"]
["","","","Niski","dBA","33","36.0","37.0"]
["Połączenia instalacji","Ciecz","","Śr. zewn.","mm","9.52","9.52","9.52"]
["","Gaz","","Śr. zewn.","mm","15.90","19.1","22.2"]
["","Spust","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Wysokość spustu","mm","","","","625"]
["Panel dekoracyjny","Model","","","","BYBS125DJW1"]
["","Kolor","","","","Biały (10Y9/0,5)"]
["","Wymiary","","Wysokość","mm","55"]
["","","","Szerokość","mm","1,500"]
["","","","Głębokość","mm","500"]
["","Ciężar","","","kg","6.5"]
["Control systems","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standardowe akcesoria","Śruby","","","","16","2","2"]
["","Podkładka","","","","8","12","12"]
["","Opaska zaciskowa przewodu elastycznego","","","","1"]
["","Przewód spustowy","","","","1"]
["","Ogólne zalecenia dotyczące bezpieczeństwa","","","","1","1","1"]
["","Instrukcja obsługi i instalacji","","","","1","1","1"]
["","Przewód dla normalnego zasilania","","","","2"]
["","Materiał uszczelniający (elastyczny przewód spustowy)","","","","1"]
["","Materiał uszczelniający","","","","2"]
["","Rura z izolacją cieplną (ciecz)","","","","1"]
["","Rura z izolacją cieplną (gaz)","","","","1"]
["Power supply","Nazwa","","","","","VE","VE"]
["","Phase","","","","1~","1~","1~"]
["","Częstotliwość","","","Hz","50/60","50/60","50/60"]
["","Napięcie","","","V","220-240/220","220-240/220","220-240/220"]
["Uwagi","","","","","(1) - Dane elektryczne, patrz oddzielny rysunek"]
["Standardowe akcesoria","Instrukcja obsługi","","","","","1","1"]
["","Instrukcja instalacji","","","","","1","1"]
["","Łącznik rurowy gazu","","","","","1","1"]
["","Materiał obejmy przewodów elektrycznych","","","","","1","1"]
["","Podkładka sprężysta","","","","","2","2"]
["","Śruba +podkładka","","","","","45","45"]
["","Śruba z łbem sześciokątnym z podkładką","","","","","49","49"]
["","Śruba z łbem sześciokątnym","","","","","2","2"]
["","Podkłada okrągła","","","","","8","8"]