{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":6,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RZQ-C"]
[]
[]
[]
[]
["","","","","FDQ200B8V3B9 / RZQ200C7Y1B","FDQ250B8V3B9 / RZQ250C7Y1B"]
["Wydajność chłodnicza","Nom.","","kW","20.0 (1)","24.1 (1)"]
["Wydajność grzewcza","Nom.","","kW","23.0 (2)","26.4 (2)"]
["Efektywność nominalna","Rocz. zużycie ener.","","kWh","3,115","4,290"]
["","COP","","","3.41","3.21"]
["","EER","","","3.21","2.81"]
["Połączenia instalacji rurowej","Gaz","Śr. zewn.","mm","22.2","22.2"]
["","Ciecz","Śr. zewn.","mm","9.52","12.70"]
["Uwagi","","","","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewnętrznej 35°CDB; długość równoważna instalacji rurowej: 5 m; różnica poziomów: 0 m","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewnętrznej 35°CDB; długość równoważna instalacji rurowej: 5 m; różnica poziomów: 0 m"]
["","","","","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 5 m; różnica poziomów: 0 m","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 5 m; różnica poziomów: 0 m"]
["","","","","(3) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)","(3) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)"]