{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RZQ-D3/D9V1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9 / RZQ125D9V1B"]
["Wydajność chłodnicza","Nom.","","kW","12.5 (3)"]
["Połączenia instalacji rurowej","Ciecz","Śr. zewn.","mm","9.52"]
["","Gaz","Śr. zewn.","mm","15.9"]
["","Spust","OD","mm","26"]
["Chłodzenie pomieszczeń","SEER","","","3.50"]
["Efektywność nominalna","Rocz. zużycie ener.","","kWh","1,978"]
["","EER","","","3.16"]
["","COP","","","3.88"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","B"]
["","","Ogrzewanie","","A"]
["Wydajność grzewcza","Nom.","","kW","14.0 (4)"]
["Uwagi","","","","(1) - Klasa energetyczna: skala od A (najwydajniejsza) do G (najmniej wydajna)"]
["","","","","(2) - Roczne zużycie energii: w oparciu na o średnią pracę urządzenia przez 500 godzin w roku przy pełnym obciążeniu (nominalne warunki)"]
["","","","","(3) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 5 m; różnica poziomów: 0 m"]
["","","","","(4) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 5 m; różnica poziomów: 0 m"]
["","","","","(5) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)"]