{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FDQ125C5VEB / RZQG125L8Y1B","FDQ125C7VEB / RZQG125L8Y1B"]
["Wydajność chłodnicza","Nom.","","kW","12.0","12.0"]
["Chłodzenie pomieszczeń","SEER","","","5.81","5.81"]
["","Roczne zużycie energii","","kWh/rok","723","723"]
["","Wydajność","Pdesign","kW","12","12"]
["","Klasa efektywności energetycznej","","","A+","A+"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Wydajność","Pdesign","kW","12.71","12.71"]
["","SCOP/A","","","4.21","4.21"]
["","Klasa efektywności energetycznej","","","A+","A+"]
["","Roczne zużycie energii","","kWh/rok","4,227","4,227"]
["Efektywność nominalna","Annual energy consumption","","kWh","1,600","1,600"]
["","EER","","","3.75","3.75"]
["","COP","","","3.83","3.83"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A","A"]
["","","Ogrzewanie","","A","A"]
["Wydajność grzewcza","Nom.","","kW","13.5","13.5"]
["Uwagi","","","","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską"]
["","","","","(2) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)","(2) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)"]