{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RXM-N"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B / RXM50N2V1B","FDXM60F3V1B / RXM60N2V1B"]
["Wydajność chłodnicza","Min.","","kW","","1.70"]
["","Nom.","","kW","","6.00"]
["","Maks.","","kW","","6.50"]
["Wydajność grzewcza","Min.","","kW","","1.70"]
["","Nom.","","kW","","7.00"]
["","Maks.","","kW","","7.10"]
["Efektywność nominalna","EER","","","","2.93"]
["","COP","","","","3.21"]
["","Rocz. zużycie ener.","","kWh","","1,024"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","","C"]
["","","Ogrzewanie","","","C"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","","A"]
["","Wydajność","Pdesign","kW","","6.00"]
["","SEER","","","","5.56"]
["","Roczne zużycie energii","","kWh/rok","","378"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","","A"]
["","Wydajność","Pdesign","kW","","4.60"]
["","SCOP/A","","","","3.80"]
["","Roczne zużycie energii","","kWh/rok","","1,693"]
["Uwagi","","","","","(1) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","","(2) - Dane elektryczne, patrz oddzielny rysunek"]
["","","","","","(3) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","","(4) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["Jednostka zewnętrzna","","","","RXM50N2V1B"]
["Wydajność chłodnicza","Min.","","kW","1.70"]
["","Nom.","","kW","5.00"]
["","Maks.","","kW","5.30"]
["Wydajność grzewcza","Min.","","kW","1.70"]
["","Nom.","","kW","5.80"]
["","Maks.","","kW","6.00"]
["Wydaj. znam.","EER","","","3.06"]
["","COP","","","3.10"]
["","Rocz. zużycie ener.","","kWh","816"]
["Efektywność nominalna","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","B"]
["","","Ogrzewanie","","D"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","A+"]
["","Wydajność","Pdesign","kW","5.00"]
["","SEER","","","5.77"]
["","Roczne zużycie energii","","kWh/rok","303"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","A"]
["","Wydajność","Pdesign","kW","4.00"]
["","SCOP/A","","","3.93"]
["","Pdh Wydajność grzewcza w temp. -10°","","kW","3.55"]
["","Roczne zużycie energii","","kWh/rok","1424"]
["Zakres efektywności energetycznej","","","","A+++ ~ D"]