{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RXS-L3"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B9 / RXS25L3V1B","FDXM35F3V1B9 / RXS35L3V1B"]
["Wydajność chłodnicza","Min.","","kW","1.30","1.40"]
["","Maks.","","kW","3.00","3.80"]
["","Nom.","","kW","2.40","3.40"]
["Piping connections","Ciecz","Śr. zewn.","mm","6.35","6.35"]
["","Gaz","Śr. zewn.","mm","9.50","9.50"]
["","Spust","OD","mm","VP20 (Średnica zewnętrzna 26, Średnica wewnętrzna 20)","VP20 (Średnica zewnętrzna 26, Średnica wewnętrzna 20)"]
["Efektywność nominalna","Rocz. zużycie ener.","","kWh","321","574"]
["","EER","","","3.74","2.96"]
["","COP","","","4.00","3.48"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A","B"]
["","","Ogrzewanie","","A","A"]
["Wydajność grzewcza","Nom.","","kW","3.20","4.00"]
["","Min.","","kW","1.30","1.40"]
["","Maks.","","kW","4.50","5.00"]
["Uwagi","","","","(1) - Nominalne wydajności chłodzenia oparte są na: temperatura wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m.","(1) - Nominalne wydajności chłodzenia oparte są na: temperatura wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m.","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["","","","","(3) - Patrz oddzielny rysunek zakresu pracy","(3) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","(4) - Dane elektryczne, patrz oddzielny rysunek","(4) - Dane elektryczne, patrz oddzielny rysunek"]