{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Poziom ciś. akust.","Grzanie","","Wysoki","dBA","35.0","35.0","","38.0"]
["","","","Czynnik","dBA","33.0","33.0","","35.0"]
["","","","Niski","dBA","27.0","27.0","","30.0"]
["","Chłodzenie","","Medium","dBA","33.0","33.0","","35.0"]
["","","","Niski","dBA","27.0","27.0","","30.0"]
["","","","Wysoki","dBA","35.0","35.0","","38.0"]
["Standardowe akcesoria","Instrukcja instalacji","","","","1","1","","1"]
["","Instrukcja obsługi","","","","1","1","","1"]
["","Izolacja mocowania","","","","1","1","","1"]
["","Podkładka uszczelniająca","","","","1","1","","1"]
["","Zacisk metalowy","","","","1","1","","1"]
["","Przewód spustowy","","","","1","1","","1"]
["","Podkładka do wspornika wieszaka","","","","8","8","","8"]
["","Materiał uszczelniający","","","","2","2","","2"]
["","Zaciski","","","","6","6","","6"]
["","Płyta mocująca z podkładką","","","","4","4","","4"]
["","Śruby dla kołnierzy przewodów","","","","1","1","","1"]
["","Filtr powietrza","","","","1","1","","1"]
["Piping connections","Ciecz","","Śr. zewn.","mm","6.35","6.35","","6.35"]
["","Gaz","","Śr. zewn.","mm","9.50","9.50","","12.70"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Power input","Chłodzenie","","Nom.","kW","0.036","0.036","","0.060"]
["","Grzanie","","Nom.","kW","0.036","0.036","","0.060"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","53.0","53.0","","56.0"]
["","Ogrzewanie","","","dBA","53.0","53.0","","56.0"]
["Wymiary","Jednostka","","Szerokość","mm","750","750","","1,150"]
["","","","Głębokość","mm","620","620","","620"]
["","","","Wysokość","mm","200","200","","200"]
["Ciężar","Jednostka","","","kg","21","21","","28"]
["Wentylator","Spręż dyspozycyjny","","Nom.","Pa","30","30","","40"]
["","Szybkość przepł. pow.","Grzanie","Wysoki","m³/min","8.7","8.7","","16.0"]
["","","","Medium","m³/min","8.0","8.0","","14.8"]
["","","","Niski","m³/min","7.3","7.3","","13.5"]
["","","Chłodzenie","Niski","m³/min","7.3","7.3","","13.5"]
["","","","Medium","m³/min","8.0","8.0","","14.8"]
["","","","Wysoki","m³/min","8.7","8.7","","16.0"]
["Power supply","Phase","","","","1~","1~","","1~"]
["","Częstotliwość","","","Hz","50","50","","50"]
["","Napięcie","","","V","220-240","220-240","","220-240"]
["Uwagi","","","","","(1) - Dane elektryczne, patrz oddzielny rysunek","(1) - Dane elektryczne, patrz oddzielny rysunek","","(1) - Dane elektryczne, patrz oddzielny rysunek"]
["Pobór mocy","Chłodzenie","","Nom.","kW","","","0.060"]
["","Grzanie","","Nom.","kW","","","0.060"]
["Wymiary","Jednostka","","Wysokość","mm","","","200"]
["","","","Szerokość","mm","","","1150"]
["","","","Głębokość","mm","","","620"]
["Ciężar","Jednostka","","","kg","","","28"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","","","15.8"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","","","14.6"]
["","","","Niski","m³/min","","","13.3"]
["","","Grzanie","Wysoki","m³/min","","","15.8"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","","","14.6"]
["","","Grzanie","Niski","m³/min","","","13.3"]
["","Spręż dyspozycyjny","","Nom.","Pa","","","40"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","","","55.0"]
["","Ogrzewanie","","","dBA","","","55.0"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","","","38.0"]
["","","","Czynnik","dBA","","","35.0"]
["","","","Niski","dBA","","","30.0"]
["","Grzanie","","Wysoki","dBA","","","38.0"]
["","Ogrzewanie","","Czynnik","dBA","","","35.0"]
["","Grzanie","","Niski","dBA","","","30.0"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","","","6.35"]
["","Gaz","","Śr. zewn.","mm","","","12.70"]
["","Spust","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Standardowe akcesoria","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Filtr powietrza","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Zasilanie energią elektryczną","liczba faz","","","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","","","50"]
["","Napięcie","","","V","","","220-240"]