{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-E / RXS-K"]
[]
[]
[]
[]
["","","","","FDXS25E7VMB / RXS25K2V1B"]
["Wydajność chłodnicza","Nom.","","kW","2.40 (3)"]
["Połączenia instalacji rurowej","Ciecz","Śr. zewn.","mm","6.35"]
["","Gaz","Śr. zewn.","mm","9.5"]
["","Spust","Śr. zew.","mm","VP20 (Średnica zewnętrzna 26, Średnica wewnętrzna 20)"]
["Efektywność nominalna","Annual energy consumption","","kWh","345"]
["","EER","","","3.48"]
["","COP","","","3.52"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A"]
["","","Ogrzewanie","","B"]
["Wydajność grzewcza","Nom.","","kW","3.20 (4)"]
["Uwagi","","","","(1) - Klasa energetyczna: skala od A (najwydajniejsza) do G (najmniej wydajna)"]
["","","","","(2) - Roczne zużycie energii: w oparciu na o średnią pracę urządzenia przez 500 godzin w roku przy pełnym obciążeniu (nominalne warunki)"]
["","","","","(3) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewnętrznej 35°CDB; długość równoważna instalacji rurowej: 5 m; różnica poziomów: 0 m"]
["","","","","(4) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 5 m; różnica poziomów: 0 m"]
["","","","","(5) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)"]