{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9 / RXS-L"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9 / RXS50L2V1B"]
["Wydajność chłodnicza","Min.","","kW","1.7"]
["","Maks.","","kW","5.3"]
["","Nom.","","kW","5.0"]
["Piping connections","Ciecz","Śr. zewn.","mm","6.35"]
["","Gaz","Śr. zewn.","mm","12.7"]
["","Spust","OD","mm","VP20 (Średnica zewnętrzna 26, Średnica wewnętrzna 20)"]
["Efektywność nominalna","Rocz. zużycie ener.","","kWh","825"]
["","EER","","","3.03"]
["","COP","","","3.10"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","B"]
["","","Ogrzewanie","","D"]
["Wydajność grzewcza","Nom.","","kW","5.8"]
["","Min.","","kW","1.7"]
["","Maks.","","kW","6.0"]
["Uwagi","","","","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską"]
["","","","","(2) - 230 V"]
["","","","","(3) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)"]