{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXM-N"]
[]
[]
[]
[]
["","","","","FFA50A2VEB / RXM50N2V1B","FFA60A2VEB / RXM60N2V1B"]
["Wydajność chłodnicza","Nom.","","kW","5.00","5.70"]
["Chłodzenie pomieszczeń","Roczne zużycie energii","","kWh/rok","","347"]
["","Wydajność","Pdesign","kW","","5.70"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Wydajność","Pdesign","kW","","3.96"]
["","Roczne zużycie energii","","kWh/rok","","1,372"]
["Efektywność nominalna","Rocz. zużycie ener.","","kWh","771","934"]
["","EER","","","3.24","3.05"]
["","COP","","","3.49","3.41"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A","B"]
["","","Ogrzewanie","","B","B"]
["Wydajność grzewcza","Nom.","","kW","5.80","7.00"]
["Uwagi","","","","(1) - Patrz oddzielny rysunek zakresu pracy","(1) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","(2) - Dane elektryczne, patrz oddzielny rysunek","(2) - Dane elektryczne, patrz oddzielny rysunek"]
["","","","","(3) - Nominalne wydajności chłodzenia oparte są na: temperatura wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m.","(3) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","(4) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m.","(4) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","","A+"]
["","SEER","","","","5.76"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","","A+"]
["","SCOP/A","","","","4.04"]