{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FFA35A2VEB / FFA35A2VEB / RZASG71M2V1B","FFA35A2VEB / FFA35A2VEB / FFA35A2VEB / RZASG100M7V1B","FFA50A2VEB / FFA50A2VEB / RZASG100M7V1B"]
["Wydajność chłodnicza","Nom.","","kW","6.80 (1)"]
["Chłodzenie pomieszczeń","SEER","","","6.12"]
["","Roczne zużycie energii","","kWh/rok","389"]
["","Wydajność","Pdesign","kW","6.80"]
["","Klasa efektywności energetycznej","","","A++"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Wydajność","Pdesign","kW","4.50"]
["","SCOP/A","","","3.84"]
["","Klasa efektywności energetycznej","","","A"]
["","Roczne zużycie energii","","kWh/rok","1,641"]
["Wydajność grzewcza","Nom.","","kW","7.50 (2)"]
["Uwagi","","","","(1) - Chłodzenie: T2: temperatura wewn. 26,6°CDB, 19,4°CWB, temp. zewn. 48°CDB [Btu/h/W]","(1) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m.","(1) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m.","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m.","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["Jednostka zewnętrzna","","","","","RZASG100M7V1B","RZASG100M7V1B"]
["Wydajność chłodnicza","Nom.","","kW","","9.50","9.50"]
["Wydajność grzewcza","Nom.","","kW","","10.8","10.8"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","","A++","A"]
["","Wydajność","Pdesign","kW","","9.50","9.50"]
["","SEER","","","","6.24","5.49"]
["","Roczne zużycie energii","","kWh/rok","","533","606"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","","A","A"]
["","Wydajność","Pdesign","kW","","6.00","6.00"]
["","SCOP/A","","","","3.82","3.90"]
["","Roczne zużycie energii","","kWh/rok","","2199","2154"]