{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":9,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB (Archived)","FFA35A2VEB (Archived)","FFA50A2VEB (Archived)","FFA60A2VEB (Archived)"]
["Obudowa","Materiał","","","","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa"]
["Wymiary","Jednostka","","Wysokość","mm","260","260","260","260"]
["","","","Szerokość","mm","575","575","575","575"]
["","","","Głębokość","mm","575","575","575","575"]
["Ciężar","Jednostka","","","kg","16.0","16.0","17.5","17.5"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","9.0","10.0","12.0","14.5"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","8.0","8.5","10.0","12.5"]
["","","","Niski","m³/min","6.5","6.5","7.5","9.5"]
["","","Grzanie","Wysoki","m³/min","9.0","10.0","12.0","14.5"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","8.0","8.5","10.0","12.5"]
["","","Grzanie","Niski","m³/min","6.5","6.5","7.5","9.5"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","48","51","56","60"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","31.0","34.0","39.0","43.0"]
["","","","Czynnik","dBA","28.5","30.5","34.0","40.0"]
["","","","Niski","dBA","25.0","25.0","27.0","32.0"]
["","Grzanie","","Wysoki","dBA","31.0","34.0","39.0","43.0"]
["","Ogrzewanie","","Czynnik","dBA","28.5","30.5","34.0","40.0"]
["","Grzanie","","Niski","dBA","25.0","25.0","27.0","32.0"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35","6.35","6.35","6.35"]
["","Gaz","","Śr. zewn.","mm","9.52","9.52","12.70","12.70"]
["","Spust","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Panel dekoracyjny","Model","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","Kolor","","","","Biały (N9.5)","Biały (N9.5)","Biały (N9.5)","Biały (N9.5)"]
["","Wymiary","","Wysokość","mm","46","46","46","46"]
["","","","Szerokość","mm","620","620","620","620"]
["","","","Głębokość","mm","620","620","620","620"]
["","Ciężar","","","kg","2.8","2.8","2.8","2.8"]
["Panel dekoracyjny 2","Model","","","","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S"]
["","Kolor","","","","Srebrny","Srebrny","Srebrny","Srebrny"]
["","Wymiary","","Wysokość","mm","46","46","46","46"]
["","","","Szerokość","mm","620","620","620","620"]
["","","","Głębokość","mm","620","620","620","620"]
["","Ciężar","","","kg","2.8","2.8","2.8","2.8"]
["Panel dekoracyjny 3","Model","","","","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1"]
["","Kolor","","","","Biały (RAL9010)","Biały (RAL9010)","Biały (RAL9010)","Biały (RAL9010)"]
["","Wymiary","","Wysokość","mm","55","55","55","55"]
["","","","Szerokość","mm","700","700","700","700"]
["","","","Głębokość","mm","700","700","700","700"]
["","Ciężar","","","kg","2.7","2.7","2.7","2.7"]
["Panel dekoracyjny 4","Model","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","Kolor","","","","Biały (RAL9010)","Biały (RAL9010)","Biały (RAL9010)","Biały (RAL9010)"]
["","Wymiary","","Wysokość","mm","55","55","55","55"]
["","","","Szerokość","mm","700","700","700","700"]
["","","","Głębokość","mm","700","700","700","700"]
["","Ciężar","","","kg","2.7","2.7","2.7","2.7"]
["Syst. kontroli","Pilot na podczerwień","","","","BRC7EB530 (standardowy panel), BRC7F530W (biały panel), BRC7F530S (szary panel)","BRC7EB530 (standardowy panel), BRC7F530W (biały panel), BRC7F530S (szary panel)","BRC7EB530 (standardowy panel), BRC7F530W (biały panel), BRC7F530S (szary panel)","BRC7EB530 (standardowy panel), BRC7F530W (biały panel), BRC7F530S (szary panel)"]
["","Pilot przewodowy","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Standardowe akcesoria","Podkładka do wspornika wieszaka","","","","8","8","8","8"]
["","Rura izolacji cieplnej","","","","2","2","2","2"]
["","Opaska zaciskowa przewodu elastycznego","","","","1","1","1","1"]
["","Przewód spustowy","","","","1","1","1","1"]
["","Instrukcja obsługi i instalacji","","","","1","1","1","1"]
["","Śruby","","","","4","4","4","4"]
["","Materiał uszczelniający","","","","4","4","4","4"]
["","Wiązania","","","","7","7","7","7"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50","50"]
["","Napięcie","","","V","220-240","220-240","220-240","220-240"]