{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RXM-N"]
[]
[]
[]
[]
["","","","","FFA50A2VEB9 / RXM50N2V1B","FFA60A2VEB9 / RXM60N2V1B"]
["Wydajność chłodnicza","Nom.","","kW","5.00"]
["Efektywność nominalna","Rocz. zużycie ener.","","kWh","772"]
["","EER","","","3.24"]
["","COP","","","3.49"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A"]
["","","Ogrzewanie","","A"]
["Wydajność grzewcza","Nom.","","kW","5.80"]
["Uwagi","","","","(1) - Nominalne wydajności chłodzenia oparte są na: temperatura wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["","","","","(3) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","(4) - Dane elektryczne, patrz oddzielny rysunek"]
["Outdoor unit","","","","","RXM60N2V1B"]
["Wydajność chłodnicza","Nom.","","kW","","5.70"]
["Wydajność grzewcza","Nom.","","kW","","7.00"]
["Wydaj. znam.","EER","","","","3.05"]
["","COP","","","","3.41"]
["","Rocz. zużycie ener.","","kWh","","934"]
["Efektywność nominalna","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","","B"]
["","","Ogrzewanie","","","B"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","","A+"]
["","Wydajność","Pdesign","kW","","5.70"]
["","SEER","","","","5.76"]
["","Roczne zużycie energii","","kWh/rok","","347"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","","A+"]
["","Wydajność","Pdesign","kW","","3.96"]
["","SCOP/A","","","","4.04"]
["","Pdh Wydajność grzewcza w temp. -10°","","kW","","3.66"]
["","Roczne zużycie energii","","kWh/rok","","1372"]
["Zakres efektywności energetycznej","","","","","A+++ ~ D"]