{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RXM-R9"]
[]
[]
[]
[]
["","","","","FFA25A2VEB9 / RXM25R5V1B9","FFA35A2VEB9 / RXM35R5V1B9"]
["Wydajność chłodnicza","Nom.","","kW","2.50","3.40"]
["Wydajność grzewcza","Nom.","","kW","3.20","4.20"]
["Efektywność nominalna","EER","","","4.57","3.81"]
["","COP","","","3.90","3.50"]
["","Annual energy consumption","","kWh","273","446"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A","A"]
["","","Ogrzewanie","","A","B"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","","A++"]
["","Wydajność","Pdesign","kW","","3.40"]
["","SEER","","","","6.38"]
["","Roczne zużycie energii","","kWh/rok","","186"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","","A+"]
["","Wydajność","Pdesign","kW","","3.10"]
["","SCOP/A","","","","4.10"]
["","Roczne zużycie energii","","kWh/rok","","1,058"]
["Uwagi","","","","(1) - Dane elektryczne, patrz oddzielny rysunek","(1) - Nominalne wydajności chłodzenia oparte są na: temperatura wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","(2) - Patrz oddzielny rysunek zakresu pracy","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["","","","","(3) - Nominalne wydajności chłodzenia oparte są na: temperatura wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m.","(3) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","(4) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m.","(4) - Dane elektryczne, patrz oddzielny rysunek"]