{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":7,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / RXM-A"]
[]
[]
[]
[]
["","","","","FHA50AVEB98 / RXM50A5V1B","FHA50AVEB99 / RXM50A5V1B","FHA60AVEB98 / RXM60A5V1B"]
["Wydajność chłodnicza","Nom.","","kW","5.00","5.00","5.7"]
["Wydajność grzewcza","Nom.","","kW","6.00","6.00","7.2"]
["Wydaj. znam.","EER","","","3.21","3.21","3.29"]
["","COP","","","3.35","3.35","3.32"]
["","Rocz. zużycie ener.","","kWh","779","779","866"]
["Efektywność nominalna","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A","A","A"]
["","","Ogrzewanie","","C","C","C"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","A+","A+","A+"]
["","Wydajność","Pdesign","kW","5.00","5.00","5.7"]
["","SEER","","","5.92","5.92","6.08"]
["","Roczne zużycie energii","","kWh/rok","295","295","328"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","A","A","A"]
["","Wydajność","Pdesign","kW","4.35","4.35","4.71"]
["","SCOP/A","","","3.86","3.86","3.87"]
["","Pdh Wydajność grzewcza w temp. -10°","","kW","3.85","3.85","4.08"]
["","Roczne zużycie energii","","kWh/rok","1577","1577","1704"]
["Uwagi","","","","","","(1) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","","","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["","","","","","","(3) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","","","(4) - Dane elektryczne, patrz oddzielny rysunek"]