{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FHA35AVEB / RXM35M3V1B9","FHA50AVEB / RXM50M3V1B9","FHA60AVEB / RXM60M3V1B9"]
["Wydajność chłodnicza","Nom.","","kW","3.40"]
["Chłodzenie pomieszczeń","SEER","","","6.24"]
["","Roczne zużycie energii","","kWh/rok","191"]
["","Wydajność","Pdesign","kW","3.40"]
["","Klasa efektywności energetycznej","","","A++"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Wydajność","Pdesign","kW","3.10"]
["","SCOP/A","","","4.43"]
["","Klasa efektywności energetycznej","","","A+"]
["","Roczne zużycie energii","","kWh/rok","979"]
["Efektywność nominalna","Rocz. zużycie ener.","","kWh","456"]
["","EER","","","3.73"]
["","COP","","","4.08"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A"]
["","","Ogrzewanie","","A"]
["Wydajność grzewcza","Nom.","","kW","4.00"]
["Uwagi","","","","(1) - Dane elektryczne, patrz oddzielny rysunek"]
["","","","","(2) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","(3) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","(4) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["Jednostka zewnętrzna","","","","","RXM50M3V1B9","RXM60M3V1B9"]
["Wydajność chłodnicza","Nom.","","kW","","5.00","5.70"]
["Wydajność grzewcza","Nom.","","kW","","6.00","7.20"]
["Wydaj. znam.","EER","","","","3.21","3.29"]
["","COP","","","","3.35","3.32"]
["","Rocz. zużycie ener.","","kWh","","780","867"]
["Efektywność nominalna","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","","B","A"]
["","","Ogrzewanie","","","C","C"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","","A+","A+"]
["","Wydajność","Pdesign","kW","","5.00","5.70"]
["","SEER","","","","5.92","6.08"]
["","Roczne zużycie energii","","kWh/rok","","295","328"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","","A","A"]
["","Wydajność","Pdesign","kW","","4.35","4.71"]
["","SCOP/A","","","","3.86","3.87"]
["","Pdh Wydajność grzewcza w temp. -10°","","kW","","3.85","4.08"]
["","Roczne zużycie energii","","kWh/rok","","1578","1704"]